{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":9,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F / 2MXM-M"]
[]
[]
[]
[]
["","","","","FDXM35F2V1B / FDXM50F2V1B / 2MXM50M2V1B","FDXM25F2V1B / FDXM50F2V1B / 2MXM50M2V1B","FDXM35F2V1B / FDXM35F2V1B / 2MXM50M2V1B","FDXM25F2V1B / FDXM25F2V1B / 2MXM50M2V1B","FDXM25F2V1B / FDXM35F2V1B / 2MXM50M2V1B"]
["Capacità di Raffrescamento","Nom.","","kW","5.00","5.00","5.00","5.00","5.00"]
["Raffrescamento ambienti","SEER","","","6.40","6.51","6.41","6.21","6.24"]
["","Consumi energetici annuali","","kWh/a","274","269","273","282","281"]
["","Capacità","Pdesign","kW","5.00","5.00","5.00","5.00","5.00"]
["","Classe di efficienza energetica","","","A++","A++","A++","A++","A++"]
["Riscaldamento ambienti (Condizioni climatiche medie)","Capacità","Pdesign","kW","4.20","4.20","4.20","4.20","4.20"]
["","SCOP/A","","","3.89","3.86","3.82","3.78","3.79"]
["","Classe di efficienza energetica","","","A","A","A","A","A"]
["","Consumi energetici annuali","","kWh/a","1,509","1,523","1,538","1,555","1,550"]
["Efficienza nominale","EER","","","3.55","3.51","3.29","3.21","3.25"]
["","Consumo energetico annuale","","kWh","704","713","761","780","770"]
["","COP","","","3.61","3.61","3.62","3.66","3.64"]
["","Classe energetica","Raffreddamento","","A","A","A","A","A"]
["","","Riscaldamento","","A","A","A","A","A"]
["Capacità di riscaldamento","Min.","","kW","5.60","5.60","5.60","5.60","5.60"]
["Note","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]