{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":7,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXF-A"]
[]
[]
[]
[]
["","","","","","2MXF40A2V1B (Archived)","2MXF50A2V1B (Archived)"]
["Dimensions","Unit","","Height","mm","550","550"]
["","","","Width","mm","765","765"]
["","","","Depth","mm","285","285"]
["Weight","Unit","","","kg","36","41"]
["Fan motor","Speed","Cooling","Super low","rpm","500","500"]
["","","Heating","Super low","rpm","320","500"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["","Heating","Ambient","Min.","°CWB","-15","-15"]
["","","","Max.","°CWB","18","18"]
["Sound pressure level","Cooling","","High","dBA","46","48"]
["","Heating","","High","dBA","48","50"]
["Refrigerant","Type","","","","R-32","R-32"]
["","Charge","","","kg","0.88","1.15"]
["","Charge","","","tCO2Eq","0.60","0.78"]
["","GWP","","","","675","675"]
["Piping connections","Piping length","OU - IU","Max.","m","20 (1)","20 (1)"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)"]
["","Level difference","IU - OU","Max.","m","15.0","15.0"]
["","","IU - IU","Max.","m","7.5","7.5"]
["","Total piping length","System","Actual","m","30","30"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["","Screw bag","","","","1","1"]
["Power supply","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-230-240","220-230-240"]
["Notes","","","","","(1) - For one room","(1) - For one room"]
["","","","","","(2) - See separate drawing for operation range","(2) - See separate drawing for operation range"]
["","","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data"]
["","","","","","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases"]
["Standard Accessories","Reducer assembly","","","","","1"]