{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXB-C"]
[]
[]
[]
[]
["","","","","","ARXB25C2V1B","ARXB25C5V1B9","ARXB35C2V1B","ARXB35C5V1B9","ARXB50CV1B","ARXB60CV1B"]
["Sound pressure level","Heating","","Nom.","dBA","","","","","51"]
["","Cooling","","Nom.","dBA","","","","","51"]
["Refrigerant","Charge","","","TCO2Eq","","","","","3.0"]
["","GWP","","","","","","","","2,087.5"]
["","Charge","","","kg","","","","","1.45"]
["","Type","","","","","","","","R-410A"]
["Dimensions","Unit","","Width","mm","","","","","855"]
["","","","Depth","mm","","","","","328"]
["","","","Height","mm","","","","","753"]
["Compressor","Type","","","","","","","","Hermetic swing"]
["Weight","Unit","","","kg","","","","","44"]
["Power supply","Phase","","","","","","","","1~"]
["","Frequency","","","Hz","","","","","50"]
["","Voltage","","","V","","","","","220-240"]
["Notes","","","","","","","","","(1) - Contains fluorinated greenhouse gases"]
["Dimensions","Unit","","Height","mm","550","550","550","550","","753"]
["","","","Width","mm","658","658","658","658","","855"]
["","","","Depth","mm","275","275","275","275","","328"]
["Weight","Unit","","","kg","28","26","30","28","","44"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","","Hermetic swing"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10","-10","-10","-10","","-10"]
["","","","Max.","°CDB","46","46","46","46","","46"]
["","Heating","Ambient","Min.","°CWB","-15","-15","-15","-15","","-15"]
["","","","Max.","°CWB","18","18","18","18","","18"]
["Sound pressure level","Cooling","","High","dBA","46","46","48","48"]
["","Heating","","High","dBA","47","47","48","48"]
["Refrigerant","Type","","","","R-410A","R-410A","R-410A","R-410A","","R-410A"]
["","Charge","","","kg","0.74","0.74","1.0","1.0","","1.45"]
["","Charge","","","tCO2Eq","1.5","1.5","2.1","2.1","","3.0"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","","2087.5"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1","1"]
["Power supply","Phase","","","","1~","1~","1~","1~","","1~"]
["","Frequency","","","Hz","50","50","50","50","","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","","220-240"]
["Piping connections","Piping length","OU - IU","Max.","m","","15","","15","","30"]
["","Additional refrigerant charge","","","kg/m","","0.02 (for piping length exceeding 10m)","","0.02 (for piping length exceeding 10m)"]
["Standard Accessories","LOT10 Energy Label","","","","","LOT10 Energy Label","","LOT10 Energy Label"]
["Sound pressure level","Cooling","","Nom.","dBA","","","","","","51"]
["","Heating","","Nom.","dBA","","","","","","51"]