{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":9,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXV-AB"]
[]
[]
[]
[]
["","","","","","ARXV25AV1B","ARXV35AV1B","ARXV50AV1B","ARXV60AV1B"]
["Sound pressure level","Cooling","","Nom.","dBA","51","53","56","58"]
["Refrigerant","Charge","","","TCO2Eq","1.7","2","3","4.3"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","0.8","0.95","1.45","2.05"]
["","Type","","","","R-410A","R-410A","R-410A","R-410A"]
["Piping connections","Level difference","IU - OU","Max.","m","10","10","10","10"]
["Dimensions","Unit","","Width","mm","776","776","955","980"]
["","","","Depth","mm","320","320","396","427"]
["","","","Height","mm","540","540","700","790"]
["Weight","Unit","","","kg","28","29","45","60"]
["Notes","","","","","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases"]