{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":10,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXB-C / ARXB-C"]
[]
[]
[]
[]
["","","","","ATXB25C2V1B / ARXB25C2V1B","ATXB25C2V1B / ARXB25C5V1B9","ATXB35C2V1B / ARXB35C2V1B","ATXB35C2V1B / ARXB35C5V1B9","ATXB50CV1B / ARXB50CV1B","ATXB60CV1B / ARXB60CV1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.3","1.3","1.630","1.750"]
["","Max.","","kW","3.0","3.0","3.8","3.8","6.200","6.500"]
["","Nom.","","kW","2.5 (2)","2.5 (2)","3.3 (2)","3.3 (2)","5.480 (2)","6.230 (2)"]
["Space cooling","SEER","","","5.93","5.93","6.02","6.02","5.93","6.09"]
["","Annual energy consumption","","kWh/a","148","148","192","192","324","359"]
["","Capacity","Pdesign","kW","2.50","2.50","3.30","3.30","5.48","6.23"]
["","Energy efficiency class","","","A+","A+","A+","A+","A+","A+"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.40","2.40","2.80","2.80","3.64","3.80"]
["","SCOP/A","","","4.01","4.01","4.04","4.04","4.27","4.06"]
["","Energy efficiency class","","","A+","A+","A+","A+","A+","A+"]
["","Annual energy consumption","","kWh/a","838","838","970","971","1,195","1,311"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5","9.5","9.5"]
["","Drain","OD","mm","18","18","18","18"]
["Nominal efficiency","EER","","","3.25 (1)","3.25 (1)","3.21 (1)","3.21 (1)","3.22 (1)","3.23 (1)"]
["","Annual energy consumption","","kWh","385","385","514","514","851","964"]
["","COP","","","4.01 (1)","4.01 (1)","3.71 (1)","3.71 (1)","3.75 (1)","3.81 (1)"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","2.8 (2)","2.8 (2)","3.5 (2)","3.5 (2)","5.620 (2)","6.400 (2)"]
["","Min.","","kW","1.3","1.3","1.3","1.3","1.170","1.200"]
["","Max.","","kW","4.0","4.0","4.8","4.8","6.600","7.100"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","","(3) - Contains fluorinated greenhouse gases","","(3) - Contains fluorinated greenhouse gases"]