{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXB-C"]
[]
[]
[]
[]
["","","","","","ATXB25C2V1B","ATXB35C2V1B","ATXB50CV1B","ATXB60CV1B"]
["Sound pressure level","Heating","","High","dBA","","","","43"]
["","","","Silent operation","dBA","","","","33"]
["","","","Low","dBA","","","","37"]
["","Cooling","","Silent operation","dBA","","","","33"]
["","","","Super high","dBA","","","","46"]
["","","","Low","dBA","","","","37"]
["","","","High","dBA","","","","43"]
["","","","Nom.","dBA","","","","41"]
["","Cooling","","Nom.","dBA","","","","41"]
["Piping connections","Drain","","","","","","","19.05"]
["Sound power level","Cooling","","","dBA","","","","61"]
["Dimensions","Unit","","Width","mm","","","","1,065"]
["","","","Depth","mm","","","","224"]
["","","","Height","mm","","","","310"]
["Casing","Colour","","","","","","","White"]
["Weight","Unit","","","kg","","","","14"]
["Power supply","Phase","","","","","","","1~"]
["","Name","","","","","","","V1"]
["","Frequency","","","Hz","","","","50"]
["","Voltage","","","V","","","","220-240"]
["Notes","","","","","","","","(1) - All units are being tested and comply to ISO 5151 (non-conducted unit) or ISO 1325 (ducted unit)."]
["Fan","Air flow rate","Cooling","Nom.","m³/min","7.6","7.7","13.32"]
["Sound pressure level","Cooling","","Nom.","dBA","33","34","38"]
["Fan","Air flow rate","Heating","Nom.","m³/min","8.0","8.4","13.32"]
["Sound pressure level","Heating","","Nom.","dBA","34","35","38"]
["Power input","Heating","","Nom.","kW","0.030","0.030"]
["Casing","Colour","","","","White","White","White"]
["Dimensions","Unit","","Height","mm","283","283","310"]
["","","","Width","mm","770","770","1065"]
["","","","Depth","mm","216","216","224"]
["Weight","Unit","","","kg","8","8","14"]
["Fan","Air flow rate","Cooling","High","m³/min","9.2","9.3","15.00"]
["","","","Low","m³/min","6.0","6.1","11.82"]
["","","","Silent operation","m³/min","4.8","4.9","10.62"]
["","","Heating","High","m³/min","9.7","10.1","15.00"]
["","","","Low","m³/min","6.3","6.7","11.82"]
["","","","Silent operation","m³/min","5.5","5.7","10.62"]
["Sound power level","Cooling","","","dBA","55","58","55"]
["","Heating","","","dBA","55","58"]
["Sound pressure level","Cooling","","High","dBA","40","41","40"]
["","","","Low","dBA","26","27","35"]
["","","","Silent operation","dBA","21","23","32"]
["","Heating","","High","dBA","40","41","40"]
["","","","Low","dBA","28","29","35"]
["","","","Silent operation","dBA","25","26","32"]
["Piping connections","Liquid","","OD","mm","6.35","6.35"]
["","Gas","","OD","mm","9.5","9.5"]
["","Drain","","","","18","18","19.05"]
["Control systems","Infrared remote control","","","","ARC470A1","ARC470A1"]
["Standard Accessories","Installation manual","","","","1","1"]
["","AA dry-cell batteries","","","","2","2"]
["","Operation manual","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Infrared remote control","","","","1","1"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Titanium apatite photocatalytic air purification filter","","","","2","2"]
["Power supply","Name","","","","V1","V1","V1"]
["","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["Sound pressure level","Cooling","","Super high","dBA","","","44"]