{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":11,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXC-C"]
[]
[]
[]
[]
["","","","","","ATXC20CV1B","ATXC25CV1B (Archived)","ATXC35CV1B (Archived)","ATXC50CV1B (Archived)","ATXC60CV1B (Archived)","ATXC71CV1B (Archived)"]
["Power input","Cooling","","Nom.","kW","0.6","0.775","1.06","1.57","1.92","2.41"]
["","Heating","","Nom.","kW","0.67","0.755","1.08","1.52","1.73","2.49"]
["Casing","Colour","","","","White","White","White","White","White","White"]
["","Material","","","","High impact polystyrene","High impact polystyrene","High impact polystyrene","High impact polystyrene","High impact polystyrene","High impact polystyrene"]
["Dimensions","Unit","","Height","mm","288","288","288","288","297","297"]
["","","","Width","mm","770","770","770","770","990","990"]
["","","","Depth","mm","234","234","234","234","273","273"]
["Weight","Unit","","","kg","9","9","9.5","9.50","13","13"]
["Fan","Air flow rate","Cooling","High","m³/min","10.8","10.8","10.8","12.2","20.4","20.4"]
["","","","Medium","m³/min","9","9","9","10","16","16"]
["","","","Low","m³/min","6.5","6.5","6.5","8.2","13.6","13.6"]
["","","","Silent operation","m³/min","5.4","5.4","5.4","7.4","10.2","10.2"]
["Sound power level","Cooling","","","dBA","54","54","55","57","60","60"]
["Sound pressure level","Cooling","","High","dBA","38","38","39","45","46","46"]
["","","","Medium","dBA","33","33","34","39","42","42"]
["","","","Low","dBA","26","26","26","33","38","38"]
["","","","Silent operation","dBA","20","20","21","29","30","30"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","OD","mm","9.52","9.52","9.52","12.7","12.7","12.7"]
["","Drain","","","","16.5","16.5","16.5","16.5","16.5","16.5"]
["Control systems","Infrared remote control","","","","ARC486A2","ARC486A2","ARC486A2","ARC486A2","ARC486A2","ARC486A2"]
["Power supply","Name","","","","V1","V1","V1","V1","V1","V1"]
["","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]