{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXD-A"]
[]
[]
[]
[]
["","","","","","ATXD25A5V1B","ATXD35A5V1B"]
["Power input","Cooling","","Nom.","kW","","0.032"]
["","Heating","","Nom.","kW","","0.032"]
["Casing","Colour","","","","","White"]
["Dimensions","Unit","","Height","mm","","286"]
["","","","Width","mm","","770"]
["","","","Depth","mm","","225"]
["Weight","Unit","","","kg","","9.00"]
["Fan","Air flow rate","Cooling","High","m³/min","","11.0"]
["","","","Medium","m³/min","","8.5"]
["","","","Low","m³/min","","6.8"]
["","","","Silent operation","m³/min","","5.4"]
["","","Heating","High","m³/min","","11.5"]
["","","","Medium","m³/min","","9.4"]
["","","","Low","m³/min","","7.7"]
["","","","Silent operation","m³/min","","6.3"]
["Sound power level","Cooling","","","dBA","","58"]
["","Heating","","","dBA","","58"]
["Sound pressure level","Cooling","","High","dBA","","43"]
["","","","Medium","dBA","","34"]
["","","","Low","dBA","","27"]
["","","","Silent operation","dBA","","20"]
["","Heating","","High","dBA","","40"]
["","","","Medium","dBA","","35"]
["","","","Low","dBA","","29"]
["","","","Silent operation","dBA","","21"]
["Piping connections","Liquid","","OD","mm","","6"]
["","Gas","","OD","mm","","9.50"]
["","Drain","","","","","18"]
["Control systems","Infrared remote control","","","","","ARC480A78"]
["","Wired remote control","","","","","BRC944B2, BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Infrared remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","Remote control holder","","","","1","1"]
["","Mounting plate","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","General safety precautions","","","","1","1"]
["Power supply","Phase","","","","","1~"]
["","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-240"]
["Notes","","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["","","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)"]
["","","","","","","(3) - See separate drawing for electrical data"]
["Sound power level","Heating","","","dBA","55"]
["","Cooling","","","dBA","55"]
["Dimensions","Unit","","Height","mm","286"]
["","","","Width","mm","770"]
["","","","Depth","mm","225"]
["Weight","Unit","","","kg","8.5"]
["Sound pressure level","Cooling","","High","dBA","40"]
["","","","Low","dBA","26"]
["","Heating","","High","dBA","40"]
["","","","Low","dBA","28"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]