{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R / ARXM-A9"]
[]
[]
[]
[]
["","","","","ATXM35R2V1B / ARXM35A5V1B9","ATXM35R5V1B / ARXM35A5V1B9"]
["Cooling capacity","Min.","","kW","1.4","1.4"]
["","Nom.","","kW","3.4","3.4"]
["","Max.","","kW","4","4"]
["Heating capacity","Min.","","kW","1.4","1.4"]
["","Nom.","","kW","4","4"]
["","Max.","","kW","5.2","5.2"]
["Nominal efficiency","EER","","","4.23","4.23"]
["","COP","","","4.04","4.04"]
["","Annual energy consumption","","kWh","402","402"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Space cooling","Energy efficiency class","","","A+++","A+++"]
["","Capacity","Pdesign","kW","3.4","3.4"]
["","SEER","","","8.55","8.55"]
["","Annual energy consumption","","kWh/a","139","139"]
["Space heating (Average climate)","Energy efficiency class","","","A+++","A+++"]
["","Capacity","Pdesign","kW","2.5","2.5"]
["","SCOP/A","","","5.1","5.1"]
["","Pdh Heating capacity at -10°","","kW","2.35","2.35"]
["","Annual energy consumption","","kWh/a","686","686"]
["Notes","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range"]
["","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data"]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]