{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":13,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R"]
[]
[]
[]
[]
["","","","","","ATXM20R2V1B §$ ATXM20R5V1B","ATXM20R2V1B","ATXM20R5V1B","ATXM25R2V1B","ATXM25R5V1B","ATXM35R2V1B","ATXM35R5V1B","ATXM50R2V1B"]
["Sound pressure level","Heating","","High","dBA","39"]
["","","","Medium","dBA","34"]
["","","","Silent operation","dBA","20"]
["","","","Low","dBA","26"]
["","Cooling","","Medium","dBA","33"]
["","","","Silent operation","dBA","19"]
["","","","Low","dBA","25"]
["","","","High","dBA","41"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2","2","2"]
["","Remote control holder","","","","1","1","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","1","1","1","1","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2","2","2"]
["","WLAN adapter kit","","","","1","1","1","1","1","1","1","1"]
["Control systems","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A67"]
["Piping connections","Liquid","","OD","mm","6.35"]
["","Gas","","OD","mm","9.50"]
["","Drain","","","","18"]
["Power input","Cooling","","Nom.","kW","0.029"]
["","Heating","","Nom.","kW","0.023"]
["Sound power level","Cooling","","","dBA","58"]
["","Heating","","","dBA","55"]
["Dimensions","Unit","","Width","mm","778"]
["","","","Depth","mm","272"]
["","","","Height","mm","295"]
["Casing","Colour","","","","White"]
["Weight","Unit","","","kg","10.0"]
["Fan","Air flow rate","Heating","High","m³/min","9.3"]
["","","","Medium","m³/min","8.2"]
["","","","Low","m³/min","6.2"]
["","","","Silent operation","m³/min","5.1"]
["","","Cooling","Low","m³/min","5.7"]
["","","","Medium","m³/min","7.5"]
["","","","High","m³/min","10.5"]
["","","","Silent operation","m³/min","4.3"]
["Power supply","Phase","","","","1~"]
["","Name","","","","V1"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["Power input","Cooling","","Nom.","kW","","0.029","0.029","0.029","0.029","0.03","0.03","0.03"]
["","Heating","","Nom.","kW","","0.023","0.023","0.022","0.022","0.027","0.027","0.032"]
["Casing","Colour","","","","","White","White","White","White","White","White","White"]
["Dimensions","Unit","","Height","mm","","295","295","295","295","295","295","299"]
["","","","Width","mm","","778","778","778","778","778","778","998"]
["","","","Depth","mm","","272","272","272","272","272","272","292"]
["Weight","Unit","","","kg","","10","10","10","10","10","10","14.5"]
["Fan","Air flow rate","Cooling","High","m³/min","","10.5","10.5","10.5","10.5","11.3","11.3","15.8"]
["","","","Medium","m³/min","","7.5","7.5","7.6","7.6","7.8","7.8","14"]
["","","","Low","m³/min","","5.7","5.7","5.7","5.7","6","6","11.4"]
["","","","Silent operation","m³/min","","4.3","4.3","4.1","4.1","4.2","4.2","8.3"]
["","","Heating","High","m³/min","","9.3","9.3","9.8","9.8","9.8","9.8","15.8"]
["","","","Medium","m³/min","","8.2","8.2","8","8","8.5","8.5","14.2"]
["","","","Low","m³/min","","6.2","6.2","6.3","6.3","6.5","6.5","12"]
["","","","Silent operation","m³/min","","5.1","5.1","4.9","4.9","4.9","4.9","10.5"]
["Sound power level","Cooling","","","dBA","","58","58","58","58","58","58","58"]
["","Heating","","","dBA","","55","55","55","55","55","55","58"]
["Sound pressure level","Cooling","","High","dBA","","41","41","41","41","45","45","44"]
["","","","Medium","dBA","","33","33","33","33","33","33","40"]
["","","","Low","dBA","","25","25","25","25","25","25","36"]
["","","","Silent operation","dBA","","19","19","19","19","19","19","27"]
["","Heating","","High","dBA","","39","39","39","39","39","39","43"]
["","","","Medium","dBA","","34","34","34","34","35","35","39"]
["","","","Low","dBA","","26","26","27","27","28","28","34"]
["","","","Silent operation","dBA","","20","20","20","20","20","20","31"]
["Piping connections","Liquid","","OD","mm","","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","OD","mm","","9.5","9.5","9.5","9.5","9.5","9.5","12.7"]
["","Drain","","","","","18","18","18","18","18","18","18"]
["Control systems","Infrared remote control","","","","","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67"]
["","Wired remote control","","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Power supply","Name","","","","","V1","V1","V1","V1","V1","V1","V1"]
["","Phase","","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","","50","50","50","50","50","50","50"]
["","Voltage","","","V","","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standard Accessories","Silver particle filter","","","","","","","","","","","1"]