{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":9,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXN-NB"]
[]
[]
[]
[]
["","","","","","ATXN25NV1B","ATXN35NV1B","ATXN50NV1B","ATXN60NV1B"]
["Sound pressure level","Heating","","High","dBA","40","","40","43"]
["","","","Silent operation","dBA","21","","32","33"]
["","","","Low","dBA","29","","35","37"]
["","Cooling","","Silent operation","dBA","21","","32","33"]
["","","","Super high","dBA","41","","44","46"]
["","","","Low","dBA","29","","35","37"]
["","","","High","dBA","40","","40","43"]
["","","","Nom.","dBA","34","","38","41"]
["","Cooling","","Nom.","dBA","34","","38","41"]
["Sound power level","Cooling","","","dBA","53","","55","61"]
["","Heating","","","dBA","53","","55","61"]
["Dimensions","Unit","","Width","mm","859","","1,124","1,124"]
["","","","Depth","mm","209","","237","237"]
["","","","Height","mm","288","","310","310"]
["Casing","Colour","","","","White","","White","White"]
["Weight","Unit","","","kg","9.0","","14.0","14.0"]
["Power supply","Phase","","","","1~","","1~","1~"]
["","Name","","","","V1","","V1","V1"]
["","Frequency","","","Hz","50","","50","50"]
["","Voltage","","","V","220-240","","220-240","220-240"]
["Notes","","","","","(1) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)","","(1) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)","(1) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)"]
["","","","","","(2) - All specifications are subjected to change by the manufacturer without prior notice.","","(2) - All specifications are subjected to change by the manufacturer without prior notice.","(2) - All specifications are subjected to change by the manufacturer without prior notice."]
["Fan","Air flow rate","Cooling","Nom.","m³/min","","7.98"]
["Sound pressure level","Cooling","","Nom.","dBA","","34"]
["Fan","Air flow rate","Heating","Nom.","m³/min","","7.98"]
["Sound pressure level","Heating","","Nom.","dBA","","34"]
["Casing","Colour","","","","","White"]
["Dimensions","Unit","","Height","mm","","288"]
["","","","Width","mm","","859"]
["","","","Depth","mm","","209"]
["Weight","Unit","","","kg","","9.0"]
["Fan","Air flow rate","Cooling","High","m³/min","","10.14"]
["","","","Low","m³/min","","6.54"]
["","","","Silent operation","m³/min","","4.68"]
["","","Heating","High","m³/min","","10.14"]
["","","","Low","m³/min","","6.54"]
["","","","Silent operation","m³/min","","4.68"]
["Sound power level","Cooling","","","dBA","","54"]
["","Heating","","","dBA","","54"]
["Sound pressure level","Cooling","","Super high","dBA","","42"]
["","","","High","dBA","","41"]
["","","","Low","dBA","","30"]
["","","","Silent operation","dBA","","22"]
["","Heating","","High","dBA","","41"]
["","","","Low","dBA","","30"]
["","","","Silent operation","dBA","","22"]
["Power supply","Name","","","","","V1"]
["","Phase","","","","","1~"]
["","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-240"]