{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":9,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXN-NB9"]
[]
[]
[]
[]
["","","","","","ATXN25NV1B9","ATXN35NV1B9","ATXN50NV1B9","ATXN60NV1B9"]
["Sound pressure level","Cooling","","Silent operation","dBA","21","22","","33"]
["","","","Super high","dBA","41","42","","46"]
["","","","Low","dBA","29","30","","37"]
["","","","High","dBA","40","41","","43"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1"]
["","Batteries","","","","Batteries","Batteries","Batteries","Batteries"]
["","Remote control holder","","","","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1"]
["","Titanium apatite filters","","","","Titanium apatite filters","Titanium apatite filters","Titanium apatite filters","Titanium apatite filters"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","","6.35"]
["","Gas","","OD","mm","9.50","9.50","","15.90"]
["","Drain","","","","16.5","16.5","","16.5"]
["Power input","Cooling","","Nom.","kW","693.00","1,060.00","","1,931.00"]
["","Heating","","Nom.","kW","700.00","950.00","","1,680.00"]
["Sound power level","Cooling","","","dBA","53","54","","61"]
["Dimensions","Unit","","Width","mm","859","859","","1,124"]
["","","","Depth","mm","209","209","","237"]
["","","","Height","mm","288","288","","310"]
["Casing","Material","","","","High impact polystyrene","High impact polystyrene","","High impact polystyrene"]
["","Colour","","","","White","White","","White"]
["Weight","Unit","","","kg","9.0","9.0","","14.0"]
["Power supply","Phase","","","","1~","1~","","1~"]
["","Name","","","","V1","V1","","V1"]
["","Frequency","","","Hz","50","50","","50"]
["","Voltage","","","V","220-240","220-240","","220-240"]
["Notes","","","","","(1) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)","(1) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)","","(1) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)"]
["","","","","","(2) - All specifications are subjected to change by the manufacturer without prior notice.","(2) - All specifications are subjected to change by the manufacturer without prior notice.","","(2) - All specifications are subjected to change by the manufacturer without prior notice."]
["Fan","Air flow rate","Cooling","Nom.","m³/min","","","13.30"]
["","","Heating","Nom.","m³/min","","","13.30"]
["Power input","Cooling","","Nom.","kW","","","1668"]
["","Heating","","Nom.","kW","","","1550"]
["Casing","Colour","","","","","","White"]
["","Material","","","","","","High impact polystyrene"]
["Dimensions","Unit","","Height","mm","","","310"]
["","","","Width","mm","","","1124"]
["","","","Depth","mm","","","237"]
["Weight","Unit","","","kg","","","14"]
["Fan","Air flow rate","Cooling","High","m³/min","","","15"]
["","","","Low","m³/min","","","11.8"]
["","","","Silent operation","m³/min","","","10.6"]
["","","Heating","High","m³/min","","","15.3"]
["","","","Low","m³/min","","","11.8"]
["","","","Silent operation","m³/min","","","10.6"]
["Sound power level","Cooling","","","dBA","","","55"]
["Sound pressure level","Cooling","","Super high","dBA","","","44"]
["","","","High","dBA","","","40"]
["","","","Low","dBA","","","35"]
["","","","Silent operation","dBA","","","32"]
["Piping connections","Liquid","","OD","mm","","","6.35"]
["","Gas","","OD","mm","","","12.7"]
["","Drain","","","","","","16.5"]
["Power supply","Name","","","","","","V1"]
["","Phase","","","","","","1~"]
["","Frequency","","","Hz","","","50"]
["","Voltage","","","V","","","220-240"]