{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXQ-A / ARXQ-A"]
[]
[]
[]
[]
["","","","","ATXQ25AMV1B / ARXQ25AMV1B","ATXQ35AMV1B / ARXQ35AMV1B"]
["Cooling capacity","Min.","","kW","1.30","1.30"]
["","Max.","","kW","3.00","3.80"]
["","Nom.","","kW","2.50","3.50"]
["Space cooling","SEER","","","6.16","6.15"]
["","Annual energy consumption","","kWh/a","142","199"]
["","Capacity","Pdesign","kW","2.50","3.50"]
["","Energy efficiency class","","","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.30","2.40"]
["","SCOP/A","","","4.15","4.11"]
["","Energy efficiency class","","","A+","A+"]
["","Pdh Heating capacity at -10°","","kW","1.81","1.90"]
["","Annual energy consumption","","kWh/a","776","818"]
["Nominal efficiency","Annual energy consumption","","kWh","386","540"]
["","EER","","","3.24","3.24"]
["","COP","","","3.71","3.71"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Heating capacity","Nom.","","kW","3.00","3.90"]
["","Min.","","kW","1.30","1.30"]
["","Max.","","kW","3.90","4.80"]