{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":7,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXQ-A"]
[]
[]
[]
[]
["","","","","","ATXQ25AMV1B","ATXQ35AMV1B"]
["Power input","Cooling","","Nom.","kW","0.023","0.025"]
["","Heating","","Nom.","kW","0.027","0.031"]
["Casing","Colour","","","","White","White"]
["Dimensions","Unit","","Height","mm","291","291"]
["","","","Width","mm","770","770"]
["","","","Depth","mm","232","232"]
["Weight","Unit","","","kg","9","9"]
["Fan","Air flow rate","Cooling","High","m³/min","10.2","10.5"]
["","","","Medium","m³/min","8.1","8.5"]
["","","","Low","m³/min","6.5","7"]
["","","","Silent operation","m³/min","5","6"]
["","","Heating","High","m³/min","11.1","12"]
["","","","Medium","m³/min","9.6","10"]
["","","","Low","m³/min","8.1","8.3"]
["","","","Silent operation","m³/min","6.8","6.9"]
["Sound power level","Cooling","","","dBA","55","55"]
["Sound pressure level","Cooling","","High","dBA","40","41"]
["","","","Medium","dBA","34","35"]
["","","","Low","dBA","26","28"]
["","","","Silent operation","dBA","23","24"]
["","Heating","","High","dBA","40","42"]
["","","","Medium","dBA","34","35"]
["","","","Low","dBA","29","30"]
["","","","Silent operation","dBA","25","25"]
["Piping connections","Liquid","","OD","mm","6.35","6.35"]
["","Gas","","OD","mm","9.5","9.5"]
["","Drain","","","","18","18"]
["Control systems","Infrared remote control","","","","ARC470A1","ARC470A1"]
["Standard Accessories","Installation manual","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Infrared remote control","","","","1","1"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Power supply","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]