{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":8,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXV-AB / ARXV-AB"]
[]
[]
[]
[]
["","","","","ATXV25AV1B / ARXV25AV1B","ATXV35AV1B / ARXV35AV1B","ATXV50AV1B / ARXV50AV1B","ATXV60AV1B / ARXV60AV1B"]
["Cooling capacity","Min.","","kW","0.6","0.6","1.26","2.53"]
["","Max.","","kW","3.2","3.9","6","6.8"]
["","Nom.","","kW","2.65","3.4","5.2","6.25"]
["Space cooling","SEER","","","5.60","5.60","5.60","5.10"]
["","Annual energy consumption","","kWh/a","166","213","325","429"]
["","Capacity","Pdesign","kW","2.65","3.40","5.20","6.25"]
["","Energy efficiency class","","","A+","A+","A+","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.80","3.20","4.50","5.80"]
["","SCOP/A","","","3.80","3.92","3.80","3.80"]
["","Energy efficiency class","","","A","A","A","A"]
["","Annual energy consumption","","kWh/a","1,032","1,143","1,658","2,137"]
["Nominal efficiency","EER","","","2.98","2.56","3.11","2.91"]
["","Annual energy consumption","","kWh","445","665","835","1,075"]
["","COP","","","3.11","3.12","3.23","2.96"]
["","Energy labeling Directive","Cooling","","C","E","B","C"]
["","","Heating","","D","D","C","D"]
["Heating capacity","Nom.","","kW","2.8","3.84","5.65","6.75"]
["","Min.","","kW","0.8","0.88","1.12","2.53"]
["","Max.","","kW","3.6","4.4","6.8","7.6"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]