{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":9,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXV-AB"]
[]
[]
[]
[]
["","","","","","ATXV25AV1B","ATXV35AV1B","ATXV50AV1B","ATXV60AV1B"]
["Sound pressure level","Cooling","","Silent operation","dBA","28","","35","39"]
["","","","Low","dBA","34","","40","42"]
["","","","High","dBA","41","","48","51"]
["","","","Nom.","dBA","39","","43","47"]
["Control systems","Infrared remote control","","","","ARC470A21","","ARC470A21","ARC470A21"]
["Piping connections","Liquid","","OD","mm","6.35","","6.35","6.35"]
["","Gas","","OD","mm","9.52","","12.7","15.9"]
["Sound power level","Cooling","","","dBA","50","","53","57"]
["Dimensions","Unit","","Width","mm","845","","940","1,007"]
["","","","Depth","mm","180","","200","219"]
["","","","Height","mm","275","","298","315"]
["Weight","Unit","","","kg","9","","12","14"]
["Power supply","Phase","","","","1~","","1~","1~"]
["","Frequency","","","Hz","50","","50","50"]
["","Voltage","","","V","220-240","","220-240","220-240"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","","8.3"]
["Sound pressure level","Cooling","","Nom.","dBA","","40"]
["Dimensions","Unit","","Height","mm","","275"]
["","","","Width","mm","","845"]
["","","","Depth","mm","","180"]
["Weight","Unit","","","kg","","9"]
["Fan","Air flow rate","Cooling","High","m³/min","","9.7"]
["","","","Low","m³/min","","6.7"]
["","","","Silent operation","m³/min","","5"]
["Sound power level","Cooling","","","dBA","","51"]
["Sound pressure level","Cooling","","High","dBA","","42"]
["","","","Low","dBA","","35"]
["","","","Silent operation","dBA","","30"]
["Piping connections","Liquid","","OD","mm","","6.35"]
["","Gas","","OD","mm","","9.52"]
["Control systems","Infrared remote control","","","","","ARC470A21"]
["Power supply","Phase","","","","","1~"]
["","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-240"]