{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":7,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BPMKS967A"]
[]
[]
[]
[]
["","","","","","BPMKS967B2B","BPMKS967B3B"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Reducer for outdoor unit side; Gas diameter 12.7","","","","1","1"]
["","Reducer for outdoor unit side; Gas diameter 15.9","","","","1","1"]
["","Reducer for outdoor unit side; Gas diameter 19.1","","","","1","1"]
["","Reducer for outdoor unit side; Liquid diameter 6.4","","","","1","1"]
["","Reducer for indoor unit side; Gas diameter 9.52","","","","1","1"]
["","Reducer for indoor unit side; Liquid diameter 12.7","","","","2","3"]
["","Reducer for indoor unit side; Liquid diameter 9.5","","","","2","3"]
["","Hanger metal","","","","4","4"]
["","Screws (M4x8)","","","","8","8"]
["","Heat insulation","","","","3","4"]
["","Binding band","","","","2","2"]
["Dimensions","Unit","","Width","mm","650","650"]
["","","","Depth","mm","350","350"]
["","","","Height","mm","180","180"]
["Weight","Unit","","","kg","7.5","8"]
["Connectable indoor unit type","","","","","20 class - 71 class","20 class - 71 class"]
["Piping connections","Outdoor unit","Liquid","Quantity","","1","1"]
["","","","ID","mm","9.5","9.5"]
["","","Gas","Quantity","mm","1","1"]
["","","","ID","mm","19.1","19.1"]
["","Indoor unit","Gas","Quantity","mm","2","3"]
["","","","ID","mm","15.9","15.9"]
["","","Liquid","ID","mm","6.4","6.4"]
["","","","Quantity","","2","3"]
["","Drain","","ID","mm","Drain processingless","Drain processingless"]
["Power input","Nom.","","","kW","0.010","0.010"]
["Power supply","Frequency","","","Hz","50","50"]
["","Voltage","","","V","230","230"]