{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":11,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BS1Q-A"]
[]
[]
[]
[]
["","","","","","BS1Q10ACV1B","BS1Q16ACV1B","BS1Q25ACV1B","BS1Q10A7V1B (Archived)","BS1Q16A7V1B (Archived)","BS1Q25A7V1B (Archived)"]
["Maximum capacity index of connectable indoor units","","","","","15 < x ≤ 100","100<x≤160","160<x≤250","15 < x ≤ 100","100<x≤160","160<x≤250"]
["Maximum number of connectable indoor units","","","","","6","8","8","6","8","8"]
["Dimensions","Unit","","Height","mm","207","207","207","207","207","207"]
["","","","Width","mm","388","388","388","388","388","388"]
["","","","Depth","mm","326","326","326","326","326","326"]
["Weight","Unit","","","kg","12","12","15","12","12","15"]
["Piping connections","Outdoor unit","Liquid","Type","","Brazing connection","Brazing connection","Brazing connection","Brazing connection","Brazing connection","Brazing connection"]
["","","","OD","mm","9.52","9.52","9.52","9.5","9.5","9.5"]
["","","Gas","Type","","Brazing connection","Brazing connection","Brazing connection","Brazing connection","Brazing connection","Brazing connection"]
["","","","OD","mm","15.9","15.9","22.2","15.9","15.9","22.2"]
["","","Discharge gas","Type","","Brazing connection","Brazing connection","Brazing connection","Brazing connection","Brazing connection","Brazing connection"]
["","","","OD","mm","12.7","12.7","19.1","12.7","12.7","19.1"]
["","Indoor unit","Liquid","Type","","Brazing connection","Brazing connection","Brazing connection","Brazing connection","Brazing connection","Brazing connection"]
["","","","OD","mm","9.52","9.52","9.52","9.5","9.5","9.5"]
["","","Gas","Type","","Brazing connection","Brazing connection","Brazing connection","Brazing connection","Brazing connection","Brazing connection"]
["","","","OD","mm","15.9","15.9","22.2","15.9","15.9","22.2"]
["Power input","Cooling","","Nom.","kW","0.005","0.005","0.005","0.005","0.005","0.005"]
["","Heating","","Nom.","kW","0.005","0.005","0.005","0.005","0.005","0.005"]
["Standard Accessories","Installation manual","","","","Installation manual","Installation manual","Installation manual","Installation manual","Installation manual","Installation manual"]
["","Insulation","","","","Insulation","Insulation","Insulation","Insulation","Insulation","Insulation"]
["","Accessory pipe","","","","Accessory pipe","Accessory pipe","Accessory pipe","Accessory pipe","Accessory pipe","Accessory pipe"]
["","Clamps","","","","Clamps","Clamps","Clamps","Clamps","Clamps","Clamps"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - In case of connecting with a 15-50 type indoor unit, use the accessory pipe to match the size of the field pipe. Be sure to braze the connection between the accessory pipe and the field pipe.","(1) - In case of connecting to a 150-160 type indoor unit, use the accessory pipe to match the size of the field pipe. Be sure to braze the connection between the accessory pipe and the field pipe.","(1) - In case of connecting to a 160-200 type indoor unit, use the accessory pipe to match the size of the field pipe. Be sure to braze the connection between the accessory pipe and the field pipe.","(1) - In case of connecting with a 15-50 type indoor unit, use the accessory pipe to match the size of the field pipe. Be sure to braze the connection between the accessory pipe and the field pipe.","(1) - In case of connecting to a 150-160 type indoor unit, use the accessory pipe to match the size of the field pipe. Be sure to braze the connection between the accessory pipe and the field pipe.","(1) - In case of connecting to a 160-200 type indoor unit, use the accessory pipe to match the size of the field pipe. Be sure to braze the connection between the accessory pipe and the field pipe."]
["","","","","","(2) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(2) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(2) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(2) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(2) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(2) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","","(3) - Maximum allowable voltage range variation between phases is 2%.","(3) - Maximum allowable voltage range variation between phases is 2%.","(3) - Maximum allowable voltage range variation between phases is 2%.","(3) - Maximum allowable voltage range variation between phases is 2%.","(3) - Maximum allowable voltage range variation between phases is 2%.","(3) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","","(4) - MCA/MFA: MCA = 1.25 x FLA","(4) - MCA/MFA: MCA = 1.25 x FLA","(4) - MCA/MFA: MCA = 1.25 x FLA","(4) - MCA/MFA: MCA = 1.25 x FLA","(4) - MCA/MFA: MCA = 1.25 x FLA","(4) - MCA/MFA: MCA = 1.25 x FLA"]
["","","","","","(5) - MFA ≤ 4 x FLA","(5) - MFA ≤ 4 x FLA","(5) - MFA ≤ 4 x FLA","(5) - MFA ≤ 4 x FLA","(5) - MFA ≤ 4 x FLA","(5) - MFA ≤ 4 x FLA"]
["","","","","","(6) - Next lower standard fuse rating minimum 15A","(6) - Next lower standard fuse rating minimum 15A","(6) - Next lower standard fuse rating minimum 15A","(6) - Next lower standard fuse rating minimum 15A","(6) - Next lower standard fuse rating minimum 15A","(6) - Next lower standard fuse rating minimum 15A"]
["","","","","","(7) - Select wire size based on the value of MCA","(7) - Select wire size based on the value of MCA","(7) - Select wire size based on the value of MCA","(7) - Select wire size based on the value of MCA","(7) - Select wire size based on the value of MCA","(7) - Select wire size based on the value of MCA"]
["","","","","","(8) - Instead of a fuse, use a circuit breaker","(8) - Instead of a fuse, use a circuit breaker","(8) - Instead of a fuse, use a circuit breaker","(8) - Instead of a fuse, use a circuit breaker","(8) - Instead of a fuse, use a circuit breaker","(8) - Instead of a fuse, use a circuit breaker"]