{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":13,"n_cols":7,"rows_kept":13,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32 / 5MXM-A"]
[]
[]
[]
[]
["","","","","","CHYHBH05AAV32 / 5MXM90A2V1B (Archived)","CHYHBH08AAV32 / 5MXM90A2V1B (Archived)"]
["Heating capacity","Nom.","","","kW","4.5","6.78 (1)"]
["COP","","","","","4.04","4.17 (1)"]
["Domestic hot water heating","General","","Declared load profile","","XL","XL"]
["","Average climate","","Water heating energy efficiency class","","A","A"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.09","3.09"]
["","","","Seasonal space heating eff. class","","A+","A+"]
["Notes","","","","","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), boiler bypassed","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), boiler bypassed"]