{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Sound pressure level","Heating","","High","dBA","38","","41"]
["","","","Silent operation","dBA","21","","21"]
["","","","Low","dBA","28","","30"]
["","Cooling","","Silent operation","dBA","21","","21"]
["","","","Low","dBA","25","","28"]
["","","","High","dBA","37","","42"]
["","","","Nom.","dBA","33"]
["","Cooling","","Nom.","dBA","31","","35"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1"]
["","Batteries","","","","2","","2"]
["","Remote control holder","","","","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Titanium apatite photocatalytic air purification filter","","","","2","","2"]
["Control systems","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Piping connections","Liquid","","OD","mm","6.35","","6.35"]
["","Gas","","OD","mm","9.5","","9.5"]
["","Drain","","","","18","","18"]
["Power input","Cooling","","Nom.","kW","0.040","","0.040"]
["","Heating","","Nom.","kW","0.040","","0.040"]
["Sound power level","Cooling","","","dBA","55","","59"]
["","Heating","","","dBA","56","","58"]
["Dimensions","Unit","","Width","mm","780","","780"]
["","","","Depth","mm","215","","215"]
["","","","Height","mm","289","","289"]
["Casing","Colour","","","","White","","White"]
["Weight","Unit","","","kg","8","","8"]
["Fan","Air flow rate","Heating","High","m³/min","","","10.1"]
["","","","Low","m³/min","","","6.3"]
["","","","Silent operation","m³/min","","","4.3"]
["","","Cooling","Low","m³/min","","","5.2"]
["","","","High","m³/min","","","9.2"]
["","","","Silent operation","m³/min","","","3.9"]
["","","","Nom.","m³/min","","","8.1"]
["","","Cooling","Nom.","m³/min","","","7.2"]
["Power supply","Phase","","","","1~","","1~"]
["","Name","","","","V1","","V1"]
["","Frequency","","","Hz","50","","50"]
["","Voltage","","","V","220-240","","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Power input","Cooling","","Nom.","kW","","0.04","","0.040"]
["","Heating","","Nom.","kW","","0.04","","0.040"]
["Casing","Colour","","","","","White","","White"]
["Dimensions","Unit","","Height","mm","","289","","289"]
["","","","Width","mm","","780","","780"]
["","","","Depth","mm","","215","","215"]
["Weight","Unit","","","kg","","8","","8.00"]
["Fan","Air flow rate","Cooling","High","m³/min","","7.9","","9.2"]
["","","","Medium","m³/min","","6.3","","7.2"]
["","","","Low","m³/min","","4.7","","5.2"]
["","","","Silent operation","m³/min","","3.9","","3.9"]
["","","Heating","High","m³/min","","9","","10.1"]
["","","","Medium","m³/min","","7.5","","8.1"]
["","","","Low","m³/min","","6","","6.3"]
["","","","Silent operation","m³/min","","4.3","","4.3"]
["Sound power level","Cooling","","","dBA","","55","","59"]
["","Heating","","","dBA","","56","","58"]
["Sound pressure level","Cooling","","High","dBA","","37","","42"]
["","","","Medium","dBA","","31","","35"]
["","","","Low","dBA","","25","","28"]
["","","","Silent operation","dBA","","21","","21"]
["","Heating","","High","dBA","","38","","41"]
["","","","Medium","dBA","","33","","36"]
["","","","Low","dBA","","28","","30"]
["","","","Silent operation","dBA","","21","","21"]
["Piping connections","Liquid","","OD","mm","","6.35","","6.35"]
["","Gas","","OD","mm","","9.5","","9.50"]
["","Drain","","","","","18","","18"]
["Control systems","Infrared remote control","","","","","ARC466A6","","ARC466A6"]
["Standard Accessories","AAA dry-cell batteries","","","","","2","","2"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["Power supply","Name","","","","","V1","","V1"]
["","Phase","","","","","1~","","1~"]
["","Frequency","","","Hz","","50","","50"]
["","Voltage","","","V","","220-240","","220-240"]