{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2CNL-A1A"]
[]
[]
[]
[]
["","","","","","D2CNL024A1AA"]
["Gas","Consumption (G20)","","Min","m³/h","0.40"]
["","","","Max","m³/h","2.50"]
["","NOx class","","","","6"]
["","NOx level (G20)","","","mg/kWh","42"]
["Central heating","Heat input Qn (net calorific value)","Nom","Min","kW","4.0"]
["","","","Max","kW","23.5"]
["","Heat input Qn (gross calorific value)","Nom","Min","kW","4.4"]
["","","","Max","kW","26.1"]
["","Output Pn at 80/60°C","","Min","kW","3.8"]
["","","","Nom","kW","22.8"]
["","Output Pnc at 50/30°C","","Min","kW","4.4"]
["","","","Nom","kW","24.0"]
["","Output at 37/30°C","","Nom","kW","4.4"]
["","Water temperature","","Max","°C","100"]
["Domestic hot water","Heat input (net calorific value) Qnw","Nom","Min","kW","4.0"]
["","","","Max","kW","25.5"]
["","Heat input (gross calorific value) Qnw","Nom","Min","kW","4.4"]
["","","","Max","kW","28.3"]
["","Temperature","","Max","°C","65"]
["Supply air","Connection","","","mm","100"]
["","Concentric","","","","Yes"]
["Flue gas","Temperature","","Max","°C","81"]
["","Connection","","","mm","60"]
["","Mass flow (G20)","","Max","kg/h","1.7"]
["Casing","Colour","","","","Titanium White (Ral9003)"]
["","Material","","","","Powder painted galvanised steel plate"]
["Dimensions","Unit","Height","Casing","mm","590"]
["","","","Width","mm","400"]
["","","","Depth","mm","256"]
["Weight","Unit","","Empty","kg","27"]
["","","","Full","kg","31"]
["Domestic hot water heating","General","","Declared load profile","","XL"]
["","","","Water heating energy efficiency class","","A"]
["Space heating","General","","Seasonal space heating eff. class","","A"]