{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCS601C51"]
[]
[]
[]
[]
["","","","","","DCS601C51."]
["Input","Type","","","","Touch panel (10 bit encoded analog input)"]
["Maximum number of connectable indoor units","","","","","64, 128 (1)"]
["Ambient temperature","Relative humidity <","","","%","85"]
["","Operation","","Min.","°C","0"]
["","","","Max.","°C","40"]
["Communication","DIII-NET","","Quantity","","1"]
["","","","Remark","","Air conditioning equipment communication line"]
["","10BASE-T","","Remark","","Web option"]
["","Ethernet","","Remark","","Port for web access and e-mail function"]
["","Input terminal","Digital","Quantity","","1"]
["","","","Remark","","Forced shutdown"]
["","","Pulse","Quantity","","3"]
["","","","Remark","","Power measuring pulse"]
["","Modem","","Remark","","Onboard modem capability"]
["","PCMCIA","","Remark","","Flash memory card"]
["","RS-232C","","Remark","","DIII-NET plus adapter"]
["Dimensions","Unit","","Width","mm","230"]
["","","","Depth","mm","107"]
["","","","Height","mm","147"]
["LCD","Type","","","","QVGA (320 x 240), 4,096 colours"]
["","Dimensions","","Width","inch","5.7"]
["Maximum number of connectable outdoor units","","","","","10, 20 (1)"]
["Power supply","Frequency","","","Hz","50/60"]
["","Voltage","","","V","100-240 (externally supplied)"]
["Notes","","","","","(1) - Combined with DCS601A51"]