{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DMS504B51"]
[]
[]
[]
[]
["","","","","","DMS504B51."]
["Ambient temperature","Relative humidity <","","","%","95"]
["","Storage","","Min.","°C","-20"]
["","","","Max.","°C","60"]
["","Operation","","Min.","°C","-10"]
["","","","Max.","°C","50"]
["Communication","Input terminal","Digital","Quantity","","1"]
["","","","Remark","","Forced shutdown"]
["","Transmission","","Medium","","Twisted pair wire"]
["","","","Speed","Kbps","78"]
["Installation","","","","","Mounted to indoor distribution board"]
["Dimensions","Unit","","Width","mm","168"]
["","","","Depth","mm","50"]
["","","","Height","mm","260"]
["Topology","","","","","FTT-10A (Free topology)"]
["Weight","Unit","","","kg","1.5"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50/60"]
["","Voltage","","","V","AC 100-240"]