{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":8,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DucoBox Energy Comfort Plus"]
[]
[]
[]
[]
["","","","","","DucoBox Energy Comfort Plus D350","DucoBox Energy Comfort Plus D450","DucoBox Energy Comfort Plus D550"]
["Article number","","","","","00004704","00004705","00004706"]
["Casing","Material","","","","Coated sheet steel + EPP","Coated sheet steel + EPP","Coated sheet steel + EPP"]
["Dimensions","Unit","","Height","mm","803","803","803"]
["","","","Width","mm","760","760","760"]
["","","","Depth","mm","584","584","584"]
["Weight","Unit","","","kg","47","47","47"]
["Fan","Air flow rate - 50Hz","Heat exchange mode","Ultra high","m³/h","350","450","550"]
["","","Bypass mode","Ultra high","m³/h","350","450","550"]
["Heat exchange system","","","","","Air to air cross flow sensible heat exchange","Air to air cross flow sensible heat exchange","Air to air cross flow sensible heat exchange"]
["Heat exchange element","","","","","v1: PP - v2: PET/Alu","v1: PP - v2: PET/Alu","v1: PP - v2: PET/Alu"]
["Connection duct diameter","mm","","","","180","180","180"]
["Operation mode","","","","","Heat exchange mode, Bypass mode, Frost protection mode","Heat exchange mode, Bypass mode, Frost protection mode","Heat exchange mode, Bypass mode, Frost protection mode"]
["SEC class","","","","","See note 2","See note 2","See note 2"]
["Maximum flow rate at 100 Pa ESP","Flow rate","","","m³/h","350","450","550"]
["Sound power level (Lwa)","dB","","","","48","49","54.0"]
["Annual electricity consumption","kWh/a","","","","217.5 (1)","254.4 (1)","315.2 (1)"]
["Annual heating saved","Average climate","","","kWh/a","4547 (1)","4512 (1)","4413 (1)"]
["","Cold climate","","","kWh/a","8895 (1)","8826 (1)","8633 (1)"]
["","Warm climate","","","kWh/a","2056 (1)","2040 (1)","1996 (1)"]
["Power supply","Phase","","","","3-core power cable with earthed plug","3-core power cable with earthed plug","3-core power cable with earthed plug"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","230","230","230"]
["Notes","","","","","(1) - Manual control (no DCV)","(1) - Manual control (no DCV)","(1) - Manual control (no DCV)"]
["","","","","","(2) - With 2 sensors (control factor 0.65): A+ ; Other: A","(2) - With 2 sensors (control factor 0.65): A+ ; Other: A","(2) - With 2 sensors (control factor 0.65): A+ ; Other: A"]
["","","","","","(3) - Dynamic airflow filter supply air (520 x 190 x 15 mm) Standard: ISO 16890 Coarse 65 % (= G4) Optional: ISO 16890 ePM1 55% (=F7) Dynamic airflow filter exhaust air (520 x 190 x 15 mm) Standard: ISO 16890 Coarse 65 % (= G4)","(3) - Dynamic airflow filter supply air (520 x 190 x 15 mm) Standard: ISO 16890 Coarse 65 % (= G4) Optional: ISO 16890 ePM1 55% (=F7) Dynamic airflow filter exhaust air (520 x 190 x 15 mm) Standard: ISO 16890 Coarse 65 % (= G4)","(3) - Dynamic airflow filter supply air (520 x 190 x 15 mm) Standard: ISO 16890 Coarse 65 % (= G4) Optional: ISO 16890 ePM1 55% (=F7) Dynamic airflow filter exhaust air (520 x 190 x 15 mm) Standard: ISO 16890 Coarse 65 % (= G4)"]