{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DucoBox Energy Comfort UK"]
[]
[]
[]
[]
["","","","","","DucoBox Energy Comfort 325 UK","DucoBox Energy Comfort D400 UK"]
["Article number","","","","","00004591","00004757"]
["Power input - 50Hz","Heat exchange mode","Nom.","Ultra high","kW","0.131 (1)"]
["","Bypass mode","Nom.","Ultra high","kW","0.131 (1)"]
["Casing","Material","","","","Coated sheet steel + EPP","Coated sheet steel + EPP"]
["Dimensions","Unit","","Height","mm","705","800"]
["","","","Width","mm","700","756"]
["","","","Depth","mm","525","583"]
["Weight","Unit","","","kg","21","47"]
["Fan","Air flow rate - 50Hz","Heat exchange mode","Ultra high","m³/h","325","400"]
["","","Bypass mode","Ultra high","m³/h","325","400"]
["","External static pressure - 50Hz","","Ultra high","Pa","100"]
["Operation range","Around unit","","","°CDB","-5°C~40°CDB, 90% RH or less"]
["Sound pressure level - 50Hz","Heat exchange mode","","Ultra high","dBA","63"]
["","Bypass mode","","Ultra high","dBA","63"]
["Heat exchange system","","","","","Air to air cross flow sensible heat exchange","Air to air cross flow sensible heat exchange"]
["Heat exchange element","","","","","PET/Polystyrene","v1: PP - v2: PET/Alu"]
["Connection duct diameter","mm","","","","Internal diameter Ø160","180"]
["Operation mode","","","","","Heat exchange mode, Bypass mode, Frost protection mode","Heat exchange mode, Bypass mode, Frost protection mode"]
["SEC class","","","","","A+","See note 2"]
["Maximum flow rate at 100 Pa ESP","Flow rate","","","m³/h","325","400"]
["Sound power level (Lwa)","dB","","","","55","55"]
["Annual electricity consumption","kWh/a","","","","117.3","231.7 (1)"]
["Annual heating saved","Average climate","","","kWh/a","4714","4515 (1)"]
["","Cold climate","","","kWh/a","9222","8833 (1)"]
["","Warm climate","","","kWh/a","2132","2042 (1)"]
["Power supply","Phase","","","","Single-phase earthed","3-core power cable with earthed plug"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","230","230"]
["Notes","","","","","(1) - At max flowrate","(1) - Manual control (no DCV)"]
["","","","","","(2) - At 250 m3/h","(2) - With 2 sensors (control factor 0.65): A+ ; Other: A"]
["","","","","","(3) - At 100 m3/h","(3) - Dynamic airflow filter supply air (520 x 190 x 15 mm) Standard: ISO 16890 Coarse 65 % (= G4) Optional: ISO 16890 ePM1 55% (=F7) Dynamic airflow filter exhaust air (520 x 190 x 15 mm) Standard: ISO 16890 Coarse 65 % (= G4)"]
["","","","","","(4) - At 325 m3/h"]
["","","","","","(5) - At 332 m3/h"]
["","","","","","(6) - At 401 m3/h"]