{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":20,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DucoBox Energy Premium UK"]
[]
[]
[]
[]
["","","","","","DucoBox Energy Premium 325 - 1ZS Right (UK)","DucoBox Energy Premium 325 - 1ZH Right (UK)","DucoBox Energy Premium 325 - 2ZS Right (UK)","DucoBox Energy Premium 325 - 2ZH Right (UK)","DucoBox Energy Premium 400 - 1ZS Right (UK)","DucoBox Energy Premium 400 - 1ZH Right (UK)","DucoBox Energy Premium 400 - 2ZS Right (UK)","DucoBox Energy Premium 325 - 1ZS Left (UK)","DucoBox Energy Premium 325 - 1ZH Left (UK)","DucoBox Energy Premium 325 - 2ZS Left (UK)","DucoBox Energy Premium 325 - 2ZH Left (UK)","DucoBox Energy Premium 400 - 1ZS Left (UK)","DucoBox Energy Premium 400 - 1ZH Left (UK)","DucoBox Energy Premium 400 - 2ZS Left (UK)","DucoBox Energy Premium 400 - 2ZH Left (UK)"]
["Article number","","","","","00004460","00004461","00004462","00004463","00004468","00004469","00004470","00004456","00004457","00004458","00004459","00004464","00004465","00004466","00004467"]
["Power input - 50Hz","Heat exchange mode","Nom.","Ultra high","kW","0.118 (1)","0.118 (1)","0.118 (1)","0.118 (1)","0.18 (1)","0.18 (1)","0.18 (1)","0.118 (1)","0.118 (1)","0.118 (1)","0.118 (1)","0.18 (1)","0.18 (1)","0.18 (1)","0.18 (1)"]
["","Bypass mode","Nom.","Ultra high","kW","0.118 (1)","0.118 (1)","0.118 (1)","0.118 (1)","0.18 (1)","0.18 (1)","0.18 (1)","0.118 (1)","0.118 (1)","0.118 (1)","0.118 (1)","0.18 (1)","0.18 (1)","0.18 (1)","0.18 (1)"]
["Casing","Material","","","","Coated sheet steel","Coated sheet steel","Coated sheet steel","Coated sheet steel","Coated sheet steel","Coated sheet steel","Coated sheet steel","Coated sheet steel","Coated sheet steel","Coated sheet steel","Coated sheet steel","Coated sheet steel","Coated sheet steel","Coated sheet steel","Coated sheet steel"]
["Dimensions","Unit","","Height","mm","957","957","957","957","957","957","957","957","957","957","957","957","957","957","957"]
["","","","Width","mm","740","740","740","740","740","740","740","740","740","740","740","740","740","740","740"]
["","","","Depth","mm","585","585","585","585","585","585","585","585","585","585","585","585","585","585","585"]
["Weight","Unit","","","kg","47","47","47","47","47","47","47","47","47","47","47","47","47","47","47"]
["Fan","Air flow rate - 50Hz","Heat exchange mode","Ultra high","m³/h","325","325","325","325","400","400","400","325","325","325","325","400","400","400","400"]
["","","Bypass mode","Ultra high","m³/h","325","325","325","325","400","400","400","325","325","325","325","400","400","400","400"]
["","External static pressure - 50Hz","","Ultra high","Pa","100","100","100","100","100","100","100","100","100","100","100","100","100","100","100"]
["Operation range","Around unit","","","°CDB","-5°C~40°CDB, 90% RH or less","-5°C~40°CDB, 90% RH or less","-5°C~40°CDB, 90% RH or less","-5°C~40°CDB, 90% RH or less","-5°C~40°CDB, 90% RH or less","-5°C~40°CDB, 90% RH or less","-5°C~40°CDB, 90% RH or less","-5°C~40°CDB, 90% RH or less","-5°C~40°CDB, 90% RH or less","-5°C~40°CDB, 90% RH or less","-5°C~40°CDB, 90% RH or less","-5°C~40°CDB, 90% RH or less","-5°C~40°CDB, 90% RH or less","-5°C~40°CDB, 90% RH or less","-5°C~40°CDB, 90% RH or less"]
["Sound pressure level - 50Hz","Heat exchange mode","","Ultra high","dBA","52","52","52","52","52.5","52.5","52.5","52","52","52","52","52.5","52.5","52.5","52.5"]
["","Bypass mode","","Ultra high","dBA","52","52","52","52","52.5","52.5","52.5","52","52","52","52","52.5","52.5","52.5","52.5"]
["Heat exchange system","","","","","Air to air cross flow sensible heat exchange","Air to air cross flow sensible heat exchange","Air to air cross flow sensible heat exchange","Air to air cross flow sensible heat exchange","Air to air cross flow sensible heat exchange","Air to air cross flow sensible heat exchange","Air to air cross flow sensible heat exchange","Air to air cross flow sensible heat exchange","Air to air cross flow sensible heat exchange","Air to air cross flow sensible heat exchange","Air to air cross flow sensible heat exchange","Air to air cross flow sensible heat exchange","Air to air cross flow sensible heat exchange","Air to air cross flow sensible heat exchange","Air to air cross flow sensible heat exchange"]
["Heat exchange element","","","","","PET/Polystyrene","PET/Polystyrene","PET/Polystyrene","PET/Polystyrene","PET/Polystyrene","PET/Polystyrene","PET/Polystyrene","PET/Polystyrene","PET/Polystyrene","PET/Polystyrene","PET/Polystyrene","PET/Polystyrene","PET/Polystyrene","PET/Polystyrene","PET/Polystyrene"]
["Connection duct diameter","mm","","","","Internal diameter Ø160 / External diameter Ø190","Internal diameter Ø160 / External diameter Ø190","Internal diameter Ø160 / External diameter Ø190","Internal diameter Ø160 / External diameter Ø190","Internal diameter Ø160 / External diameter Ø190","Internal diameter Ø160 / External diameter Ø190","Internal diameter Ø160 / External diameter Ø190","Internal diameter Ø160 / External diameter Ø190","Internal diameter Ø160 / External diameter Ø190","Internal diameter Ø160 / External diameter Ø190","Internal diameter Ø160 / External diameter Ø190","Internal diameter Ø160 / External diameter Ø190","Internal diameter Ø160 / External diameter Ø190","Internal diameter Ø160 / External diameter Ø190","Internal diameter Ø160 / External diameter Ø190"]
["Operation mode","","","","","Heat exchange mode, Bypass mode, Frost protection mode","Heat exchange mode, Bypass mode, Frost protection mode","Heat exchange mode, Bypass mode, Frost protection mode","Heat exchange mode, Bypass mode, Frost protection mode","Heat exchange mode, Bypass mode, Frost protection mode","Heat exchange mode, Bypass mode, Frost protection mode","Heat exchange mode, Bypass mode, Frost protection mode","Heat exchange mode, Bypass mode, Frost protection mode","Heat exchange mode, Bypass mode, Frost protection mode","Heat exchange mode, Bypass mode, Frost protection mode","Heat exchange mode, Bypass mode, Frost protection mode","Heat exchange mode, Bypass mode, Frost protection mode","Heat exchange mode, Bypass mode, Frost protection mode","Heat exchange mode, Bypass mode, Frost protection mode","Heat exchange mode, Bypass mode, Frost protection mode"]
["SEC class","","","","","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["Maximum flow rate at 100 Pa ESP","Flow rate","","","m³/h","327","327","327","327","405","405","405","327","327","327","327","405","405","405","405"]
["Sound power level (Lwa)","dB","","","","41","41","41","41","46","46","46","41","41","41","41","46","46","46","46"]
["Annual electricity consumption","kWh/a","","","","112.4","112.4","112.4","112.4","127.5","127.5","127.5","112.4","112.4","112.4","112.4","127.5","127.5","127.5","127.5"]
["Annual heating saved","Average climate","","","kWh/a","4673","4673","4673","4673","4652","4652","4652","4673","4673","4673","4673","4652","4652","4652","4652"]
["","Cold climate","","","kWh/a","9141","9141","9141","9141","9100","9100","9100","9141","9141","9141","9141","9100","9100","9100","9100"]
["","Warm climate","","","kWh/a","2113","2113","2113","2113","2104","2104","2104","2113","2113","2113","2113","2104","2104","2104","2104"]
["Power supply","Phase","","","","Single-phase earthed","Single-phase earthed","Single-phase earthed","Single-phase earthed","Single-phase earthed","Single-phase earthed","Single-phase earthed","Single-phase earthed","Single-phase earthed","Single-phase earthed","Single-phase earthed","Single-phase earthed","Single-phase earthed","Single-phase earthed","Single-phase earthed"]
["","Frequency","","","Hz","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230"]
["Notes","","","","","(1) - At max flowrate","(1) - At max flowrate","(1) - At max flowrate","(1) - At max flowrate","(1) - At max flowrate","(1) - At max flowrate","(1) - At max flowrate","(1) - At max flowrate","(1) - At max flowrate","(1) - At max flowrate","(1) - At max flowrate","(1) - At max flowrate","(1) - At max flowrate","(1) - At max flowrate","(1) - At max flowrate"]
["","","","","","(2) - At 250 m3/h","(2) - At 250 m3/h","(2) - At 250 m3/h","(2) - At 250 m3/h","(2) - At 250 m3/h","(2) - At 250 m3/h","(2) - At 250 m3/h","(2) - At 250 m3/h","(2) - At 250 m3/h","(2) - At 250 m3/h","(2) - At 250 m3/h","(2) - At 250 m3/h","(2) - At 250 m3/h","(2) - At 250 m3/h","(2) - At 250 m3/h"]
["","","","","","(3) - At 100 m3/h","(3) - At 100 m3/h","(3) - At 100 m3/h","(3) - At 100 m3/h","(3) - At 100 m3/h","(3) - At 100 m3/h","(3) - At 100 m3/h","(3) - At 100 m3/h","(3) - At 100 m3/h","(3) - At 100 m3/h","(3) - At 100 m3/h","(3) - At 100 m3/h","(3) - At 100 m3/h","(3) - At 100 m3/h","(3) - At 100 m3/h"]
["","","","","","(4) - At 325 m3/h","(4) - At 325 m3/h","(4) - At 325 m3/h","(4) - At 325 m3/h","(4) - At 325 m3/h","(4) - At 325 m3/h","(4) - At 325 m3/h","(4) - At 325 m3/h","(4) - At 325 m3/h","(4) - At 325 m3/h","(4) - At 325 m3/h","(4) - At 325 m3/h","(4) - At 325 m3/h","(4) - At 325 m3/h","(4) - At 325 m3/h"]
["","","","","","(5) - At 332 m3/h","(5) - At 332 m3/h","(5) - At 332 m3/h","(5) - At 332 m3/h","(5) - At 332 m3/h","(5) - At 332 m3/h","(5) - At 332 m3/h","(5) - At 332 m3/h","(5) - At 332 m3/h","(5) - At 332 m3/h","(5) - At 332 m3/h","(5) - At 332 m3/h","(5) - At 332 m3/h","(5) - At 332 m3/h","(5) - At 332 m3/h"]
["","","","","","(6) - At 401 m3/h","(6) - At 401 m3/h","(6) - At 401 m3/h","(6) - At 401 m3/h","(6) - At 401 m3/h","(6) - At 401 m3/h","(6) - At 401 m3/h","(6) - At 401 m3/h","(6) - At 401 m3/h","(6) - At 401 m3/h","(6) - At 401 m3/h","(6) - At 401 m3/h","(6) - At 401 m3/h","(6) - At 401 m3/h","(6) - At 401 m3/h"]