{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DucoBox Energy Sky UK"]
[]
[]
[]
[]
["","","","","","DucoBox Energy Sky D275 UK"]
["Article number","","","","","00004940"]
["Casing","Material","","","","Expanded Polypropylene + Polystyrene"]
["Dimensions","Unit","","Height","mm","1180"]
["","","","Width","mm","670"]
["","","","Depth","mm","295"]
["Weight","Unit","","","kg","19"]
["Fan","Air flow rate - 50Hz","Heat exchange mode","Ultra high","m³/h","275"]
["","","Bypass mode","Ultra high","m³/h","275"]
["Heat exchange system","","","","","Air to air cross flow heat exchange"]
["Heat exchange element","","","","","v1: PP - v2: PET/Alu"]
["Connection duct diameter","mm","","","","Internal diameter Ø160"]
["Operation mode","","","","","Heat exchange mode, Bypass mode, Frost protection mode"]
["SEC class","","","","","A+ (1)"]
["Maximum flow rate at 100 Pa ESP","Flow rate","","","m³/h","275"]
["Sound power level (Lwa)","dB","","","","45"]
["Annual electricity consumption","kWh/a","","","","115.8"]
["Annual heating saved","Average climate","","","kWh/a","4620 (2)"]
["","Cold climate","","","kWh/a","9038 (2)"]
["","Warm climate","","","kWh/a","2089 (2)"]
["Power supply","Phase","","","","3-core power cable with earthed plug"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","230"]
["Notes","","","","","(1) - With 2 sensors (control factor 0.65): A+ ; Other: A"]
["","","","","","(2) - Manual control (no DCV)"]