{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBLA04-08EV3"]
[]
[]
[]
[]
["","","","","","EBLA04E2V3","EBLA06E2V3","EBLA08E2V3"]
["Heating capacity","Nom.","","","kW","4.30 (1), 4.60 (2)","6.00 (1), 5.90 (2)","7.50 (1), 7.80 (2)"]
["Cooling capacity","Nom.","","","kW","4.86 (1), 4.52 (2)","5.83 (1), 5.09 (2)","6.18 (1), 5.44 (2)"]
["Power input","Cooling","","Nom.","kW","0.820 (1), 1.36 (2)","1.08 (1), 1.55 (2)","1.19 (1), 1.73 (2)"]
["","Heating","","Nom.","kW","0.840 (1), 1.26 (2)","1.24 (1), 1.69 (2)","1.63 (1), 2.23 (2)"]
["COP","","","","","5.10 (1), 3.65 (2)","4.85 (1), 3.50 (2)","4.60 (1), 3.50 (2)"]
["EER","","","","","5.91 (1), 3.32 (2)","5.40 (1), 3.28 (2)","5.19 (1), 3.14 (2)"]
["Dimensions","Unit","","Height","mm","770","770","770"]
["","","","Width","mm","1250","1250","1250"]
["","","","Depth","mm","362","362","362"]
["Weight","Unit","","","kg","88","88","88"]
["Operation range","Heating","Water side","Min.","°C","9 (3)","9 (3)","9 (3)"]
["","","","Max.","°C","65 (3)","65 (3)","65 (3)"]
["","Cooling","Ambient","Min.","°CDB","10 (3)","10 (3)","10 (3)"]
["","","","Max.","°CDB","43","43","43"]
["","","Water side","Min.","°C","5 (3)","5 (3)","5 (3)"]
["","","","Max.","°C","22","22","22"]
["","Domestic hot water","Ambient","Min.","°CDB","-27","-27","-27"]
["","","","Max.","°CDB","35","35","35"]
["","","Water side","Min.","°C","25","25","25"]
["","","","Max.","°C","55 (3)","55 (3)","55 (3)"]
["Sound power level","Heating","","Nom.","dBA","58.0 (1)","60.0 (1)","62.0 (1)"]
["","Cooling","","Nom.","dBA","61.0 (1)","62.0 (1)","62.0 (1)"]
["Sound pressure level","Heating","","Nom.","dBA","44.0 (1)","47.0 (1)","49.0 (1)"]
["","Cooling","","Nom.","dBA","48.0 (1)","49.0 (1)","50.0 (1)"]
["Refrigerant","Type","","","","R-32","R-32","R-32"]
["","GWP","","","","675","675","675"]
["","Charge","","","kg","1.35","1.35","1.35"]
["","Charge","","","tCO2Eq","0.91","0.91","0.91"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.29","3.28","3.35"]
["","","","Seasonal space heating eff. class","","A++","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.54","4.52","4.61"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++"]
["Compressor component","Main power supply","","Phase","","3N~","3N~","3N~"]
["","","","Voltage","V","220","220","220"]
["Power supply","Name","","","","V3","V3","V3"]
["","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","230 +/-10%","230 +/-10%","230 +/-10%"]
["Notes","","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["","","","","","(3) - For more details, see operation range drawing","(3) - For more details, see operation range drawing","(3) - For more details, see operation range drawing"]