{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":13,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSHB-D / ERLA11-14DW1"]
[]
[]
[]
[]
["","","","","","EBSHB11P30DF / ERLA11D2W1","EBSHB11P50DF / ERLA11D2W1","EBSHB11P30DF / ERLA11DAW1","EBSHB11P50DF / ERLA11DAW1","EBSHB16P30DF / ERLA14D2W1","EBSHB16P50DF / ERLA14D2W1","EBSHB16P30DF / ERLA14DAW1","EBSHB16P50DF / ERLA14DAW1"]
["Indoor unit","","","","","EBSHB11P30DF","EBSHB11P50DF","EBSHB11P30DF","EBSHB11P50DF","EBSHB16P30DF","EBSHB16P50DF","EBSHB16P30DF","EBSHB16P50DF"]
["Heating capacity","Nom.","","","kW","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","12.0 (1)","12.0 (1)","12.0 (1)","12.0 (1)"]
["Power input","Heating","","Nom.","kW","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)"]
["COP","","","","","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)"]
["Domestic hot water heating","General","","Declared load profile","","L","XL","L","XL","L","XL","L","XL"]
["","Average climate","","Water heating energy efficiency class","","A+","A+","A+","A+","A+","A+","A+","A+"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.23","3.23","3.23","3.23","3.22","3.22","3.22","3.22"]
["","","","Seasonal space heating eff. class","","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.63","4.63","4.63","4.63","4.60","4.60","4.60","4.60"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Notes","","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]