{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":12,"n_cols":12,"rows_kept":12,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ECONO-AY1"]
[]
[]
[]
[]
["","","","","","ECONO250AMY1","ECONO350AMY1","ECONO450AMY1","ECONO550AMY1","ECONO600AMY1","ECONO700AMY1","ECONO900AMY1"]
["Option for","","","","","UATYQ250CY1","UATYQ350CY1","UATYQ450CY1","UATYQ550CY1","UATYQ600CY1","UATYQ700CY1","UATYQ900CY1"]
["Weight","Unit","","","kg","51","42","43","53","54","69","78"]
["Fan","Air flow rate","Cooling","Nom.","l/s","1,560","2,030","2,670","3,160","3,445","3,917","4,533"]
["","","","Nom.","cfm","3,300","4,300","5,650","6,700","7,300","8,300","9,604.5"]
["Test Standard","","","","","ISO 13253","ISO 13253","ISO 13253","ISO 13253","ISO 13253","ISO 13253","ISO 13253"]
["Power supply","Voltage","","","V","24 DC","24 DC","24 DC","24 DC","24 DC","24 DC","24 DC"]