{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EDLA-DW17"]
[]
[]
[]
[]
["","","","","","EDLA16DAW17"]
["Heating capacity","Nom.","","","kW","16.0"]
["Power input","Heating","","Nom.","kW","3.53, 4.56"]
["COP","","","","","4.53, 3.51"]
["Dimensions","Unit","","Height","mm","870"]
["","","","Width","mm","1380"]
["","","","Depth","mm","460"]
["Weight","Unit","","","kg","147"]
["Fan","Air flow rate","Heating","High","m³/min","85.0"]
["Operation range","Heating","Water side","Min.","°C","9"]
["","","","Max.","°C","60"]
["","Domestic hot water","Ambient","Min.","°CDB","-25"]
["","","","Max.","°CDB","35"]
["","","Water side","Min.","°C","25"]
["","","","Max.","°C","55"]
["Refrigerant","Type","","","","R-32"]
["","GWP","","","","675"]
["","Charge","","","kg","3.80"]
["","Charge","","","tCO2Eq","2.57"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.33"]
["","","","Seasonal space heating eff. class","","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.62"]
["","","","Seasonal space heating eff. class","","A+++"]
["Compressor component","Main power supply","","Phase","","3N~"]
["","","","Voltage","V","400"]
["Power supply","Name","","","","W1"]
["","Phase","","","","3~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","400"]
["Notes","","","","","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]
["","","","","","(3) - For more details, see operation range drawing"]
["","","","","","(4) - Depends on operation mode, refer to installation manual."]