{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EDLA09-14D3W1"]
[]
[]
[]
[]
["","","","","","EDLA09DA3W1","EDLA11DA3W1","EDLA14DA3W1"]
["Heating capacity","Nom.","","","kW","9.37 (1), 9.00 (2)","10.6 (1), 9.82 (2)","12.0 (1), 12.5 (2)"]
["Heater capacity","Step 1","","","kW","3","3","3"]
["Power input","Heating","","Nom.","kW","1.91 (1), 2.43 (2)","2.18 (1), 2.68 (2)","2.46 (1), 3.42 (2)"]
["COP","","","","","4.91 (1), 3.71 (2)","4.83 (1), 3.66 (2)","4.87 (1), 3.64 (2)"]
["Dimensions","Unit","","Height","mm","870","870","870"]
["","","","Width","mm","1380","1380","1380"]
["","","","Depth","mm","460","460","460"]
["Weight","Unit","","","kg","149","149","149"]
["Fan","Air flow rate","Heating","High","m³/min","48.0","55.8","70.4"]
["Operation range","Heating","Water side","Min.","°C","15 (6)","15 (6)","15 (6)"]
["","","","Max.","°C","60 (6)","60 (6)","60 (6)"]
["","Domestic hot water","Ambient","Min.","°CDB","-25","-25","-25"]
["","","","Max.","°CDB","35","35","35"]
["","","Water side","Min.","°C","25","25","25"]
["","","","Max.","°C","55 (6)","55 (6)","55 (6)"]
["Refrigerant","Type","","","","R-32","R-32","R-32"]
["","GWP","","","","675","675","675"]
["","Charge","","","kg","3.80","3.80","3.80"]
["","Charge","","","tCO2Eq","2.57","2.57","2.57"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.39","3.32","3.37"]
["","","","Seasonal space heating eff. class","","A++","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.72","4.64","4.62"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Compressor component","Main power supply","","Phase","","3N~","3N~","3N~"]
["","","","Voltage","V","400","400","400"]
["Power supply","Name","","","","W1","W1","W1"]
["","Phase","","","","3~","3~","3~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","400","400","400"]
["Notes","","","","","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]
["","","","","","(3) - For more details, see operation range drawing","(3) - For more details, see operation range drawing","(3) - For more details, see operation range drawing"]
["","","","","","(4) - Depends on operation mode, refer to installation manual.","(4) - Depends on operation mode, refer to installation manual.","(4) - Depends on operation mode, refer to installation manual."]