{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSAX-D9WG"]
[]
[]
[]
[]
["","","","","","EGSAX06DA9WG","EGSAX10DA9WG"]
["Heating capacity","Min.","","","kW","0.85"]
["","Nom.","","","kW","3.35"]
["","Max.","","","kW","7.98"]
["Power input","Nom.","","","kW","0.74"]
["COP","","","","","4.51"]
["Casing","Colour","","","","Grey + Black"]
["Dimensions","Unit","","Height","mm","1,891"]
["","","","Width","mm","597"]
["","","","Depth","mm","666"]
["Weight","Unit","","","kg","222"]
["Tank","Water volume","","","l","180"]
["","Insulation","","Heat loss","kWh/24h","1.2"]
["","Corrosion protection","","","","Pickling"]
["Refrigerant","Type","","","","R-32"]
["","GWP","","","","675.0"]
["","Charge","","","kg","1.70"]
["Operation range","Installation space","","Min.","°C","5"]
["","","","Max.","°C","35"]
["","Brine side","","Min.","°C","-10"]
["","","","Max.","°C","30"]
["","Heating","Water side","Min.","°C","5"]
["","","","Max.","°C","65"]
["","Domestic hot water","Water side","Min.","°C","25"]
["","","","Max.","°C","60"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.77 (1)"]
["","","","Seasonal space heating eff. class","","A++"]
["","Average climate water outlet 35°C","General","SCOP","","5.18 (1)"]
["","","","Seasonal space heating eff. class","","A+++"]
["Power supply","Phase","","","","1~/3~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","230/400"]
["Current","Recommended fuses","","","A","16/32"]
["Notes","","","","","(1) - According to EN14825 and EN14511:2018"]
["","","","","","(2) - See operation range drawing: range increase by support booster heater or backup heater"]
["Heating capacity","Min.","","","kW","","0.85"]
["","Nom.","","","kW","","5.49"]
["","Max.","","","kW","","9.55"]
["Power input","Nom.","","","kW","","1.17"]
["COP","","","","","","4.7"]
["Casing","Colour","","","","","Grey + Black"]
["Dimensions","Unit","","Height","mm","","1891"]
["","","","Width","mm","","597"]
["","","","Depth","mm","","666"]
["Weight","Unit","","","kg","","222"]
["Tank","Insulation","","Heat loss","kWh/24h","","1.2"]
["","Corrosion protection","","","","","Pickling"]
["Refrigerant","Type","","","","","R-32"]
["","GWP","","","","","675.0"]
["","Charge","","","tCO2Eq","","1.15"]
["","Charge","","","kg","","1.70"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","","4.05 (1)"]
["","","","Seasonal space heating eff. class","","","A+++"]
["","Average climate water outlet 35°C","General","SCOP","","","5.20 (1)"]
["","","","Seasonal space heating eff. class","","","A+++"]
["Power supply","Phase","","","","","1~/3~"]
["","Frequency","","","Hz","","50"]
["","Voltage","","","V","","230/400"]
["Current","Recommended fuses","","","A","","16/32"]
["Notes","","","","","","(1) - According to EN14825 and EN14511:2018"]