{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":7,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSAX-UD9W"]
[]
[]
[]
[]
["","","","","","EGSAX06UDA9W","EGSAX10UDA9W"]
["Refrigerant","GWP","","","","675.0","675.0"]
["","Charge","","","kg","1.70","1.70"]
["","Type","","","","R-32","R-32"]
["Operation range","Installation space","","Min.","°C","5","5"]
["","","","Max.","°C","35","35"]
["","Heating","Water side","Max.","°C","65","65"]
["","","","Min.","°C","5","5"]
["","Brine side","","Min.","°C","-10","-10"]
["","","","Max.","°C","30","30"]
["","Domestic hot water","Water side","Max.","°C","60","60"]
["","","","Min.","°C","25","25"]
["Power input","Nom.","","","kW","0.74","1.17"]
["COP","","","","","4.51","4.70"]
["Dimensions","Unit","","Width","mm","597","597"]
["","","","Depth","mm","666","666"]
["","","","Height","mm","1,891","1,891"]
["Casing","Material","","","","Precoated sheet metal"]
["","Colour","","","","White + Black","White + Black"]
["Tank","Water volume","","","l","180","180"]
["","Corrosion protection","","","","Pickling","Pickling"]
["","Insulation","","Heat loss","kWh/24h","1.35","1.35"]
["Weight","Unit","","","kg","222","222"]
["Space heating","Average climate water outlet 35°C","General","ηs (Seasonal space heating efficiency)","%","199","200"]
["","","","Seasonal space heating eff. class","","A+++","A+++"]
["","","","SCOP","","5.18 (1)","5.20 (1)"]
["","Average climate water outlet 55°C","General","Seasonal space heating eff. class","","A++","A+++"]
["","","","ηs (Seasonal space heating efficiency)","%","143","154"]
["","","","SCOP","","3.77 (1)","4.05 (1)"]
["Heating capacity","Nom.","","","kW","3.35","5.49"]
["","Min.","","","kW","0.85","0.85"]
["","Max.","","","kW","7.98","9.55"]
["Power supply","Phase","","","","1~/3~","1~/3~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","230/400","230/400"]
["Current","Recommended fuses","","","A","16/32","16/32"]
["Notes","","","","","(1) - According to EN14825 and EN14511:2018","(1) - According to EN14825 and EN14511:2018"]
["","","","","","(2) - See operation range drawing: range increase by support booster heater or backup heater","(2) - See operation range drawing: range increase by support booster heater or backup heater"]