{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBH-CBV"]
[]
[]
[]
[]
["","","","","","EHBH04CBV","EHBH08CBV","EHBH11CBV","EHBH16CBV"]
["Casing","Colour","","","","White","White","White","White"]
["","Material","","","","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal"]
["Dimensions","Unit","","Height","mm","890","890","890","890"]
["","","","Width","mm","480","480","480","480"]
["","","","Depth","mm","344","344","344","344"]
["Weight","Unit","","","kg","39.0","41.0","41.0","42.0"]
["PED","Category","","","","Art3§3, See note 1","Category I, See note 1","Art3§3, See note 1","Art3§3, See note 1"]
["Sound power level","Nom.","","","dBA","40.0","40.0","41.0","44.0"]
["Sound pressure level","Nom.","","","dBA","26.0","26.0","27.0","30.0"]
["Operation range","Heating","Water side","Min.","°C","10","10","10","10"]
["","","","Max.","°C","55.0","55.0","55.0","55.0"]
["Power supply","Name","","","","See note 12","See note 12","See note 12","See note 12"]
["Wiring connections","For connection with user interface","","Quantity","","2","2","2","2"]
["","","","Remark","","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)"]
["Notes","","","","","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation)."]
["","","","","","(2) - Including piping + PHE + back-up heater; excluding expansion vessel","(2) - Including piping + PHE + back-up heater; excluding expansion vessel","(2) - Including piping + PHE + back-up heater; excluding expansion vessel","(2) - Including piping + PHE + back-up heater; excluding expansion vessel"]
["","","","","","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)"]
["","","","","","(4) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.The sound pressure level mentioned is maximum possible value inside operation range of unit.","(4) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.The sound pressure level mentioned is maximum possible value inside operation range of unit.","(4) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.The sound pressure level mentioned is maximum possible value inside operation range of unit.","(4) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.The sound pressure level mentioned is maximum possible value inside operation range of unit."]
["","","","","","(5) - Lower if back-up heater is installed; In case of no back-up heater, then heat pump operation starts at 10°C","(5) - Lower if back-up heater is installed; In case of no back-up heater, then heat pump operation starts at 10°C","(5) - Lower if back-up heater is installed; In case of no back-up heater, then heat pump operation starts at 10°C","(5) - Lower if back-up heater is installed; In case of no back-up heater, then heat pump operation starts at 10°C"]
["","","","","","(6) -  > 50°C BSH only, no heatpump","(6) -  > 50°C BSH only, no heatpump","(6) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models","(6) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models"]
["","","","","","","","(7) -  > 50°C BSH only, no heatpump","(7) -  > 50°C BSH only, no heatpump"]