{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":62,"n_cols":9,"rows_kept":62,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHOBG-A"]
[]
[]
[]
[]
["","","","","","EHOBG12ABV1","EHOBG18ABV1","EHOBG12AAV1","EHOBG18AAV1"]
["Gas","Connection","","Diameter","mm","","","","15"]
["","Consumption (G20)","","Min","m³/h","","","","0.58"]
["","","","Max","m³/h","","","","1.94"]
["","Consumption (G25)","","Min","m³/h","","","","0.67"]
["","","","Max","m³/h","","","","2.25"]
["","Consumption (G31)","","Min","m³/h","","","","0.22"]
["","","","Max","m³/h","","","","0.74"]
["","NOx class","","","","","","","6"]
["","NOx level (G20)","","","mg/kWh","","","","28"]
["Central heating","Heat input Qn (net calorific value)","Nom","Min","kW","","","","5.6"]
["","","","Max","kW","","","","18.7"]
["","Heat input Qn (gross calorific value)","Nom","Min","kW","","","","6.2"]
["","","","Max","kW","","","","20.8"]
["","Output Pn at 80/60°C","","Nom","kW","","","","18.2"]
["","Output at 37/30°C","","Nom","kW","","","","6.1"]
["","Water temperature","","Max","°C","","","","90"]
["Space heating","General","","ηs (Seasonal space heating efficiency)","%","","","","92"]
["","","","Seasonal space heating eff. class","","","","","A"]
["Supply air","Concentric","","","","","","","60/100"]
["Flue gas","Temperature","","Max","°C","","","","70"]
["","Mass flow (G20)","","Max","kg/h","","","","31.3"]
["","Mass flow (G25)","","Max","kg/h","","","","31.3"]
["","Mass flow (G31)","","Max","kg/h","","","","30.6"]
["Casing","Colour","","","","","","","RAL9010"]
["","Material","","","","","","","Precoated sheet metal"]
["Dimensions","Unit","Height","Casing","mm","","","","590"]
["Gas","Connection","","Diameter","mm","15","15","15"]
["","Consumption (G20)","","Min","m³/h","0.36","0.58","0.36"]
["","","","Max","m³/h","1.30","1.94","1.30"]
["","Consumption (G25)","","Min","m³/h","0.42","0.67","0.42"]
["","","","Max","m³/h","1.50","2.25","1.50"]
["","Consumption (G31)","","Min","m³/h","0.14","0.22","0.14"]
["","","","Max","m³/h","0.49","0.74","0.49"]
["","NOx class","","","","6","6","6"]
["","NOx level (G20)","","","mg/kWh","28","28","28"]
["Central heating","Heat input Qn (net calorific value)","Nom","Min","kW","3.8","5.6","3.8"]
["","","","Max","kW","12.5","18.7","12.5"]
["","Heat input Qn (gross calorific value)","Nom","Min","kW","4.2","6.2","4.2"]
["","","","Max","kW","13.9","20.8","13.9"]
["","Output Pn at 80/60°C","","Nom","kW","12.2","18.2","12.2"]
["","Output at 37/30°C","","Nom","kW","4.1","6.1","4.1"]
["","Water temperature","","Max","°C","90","90","90"]
["Supply air","Concentric","","","","60/100","60/100","60/100"]
["Flue gas","Temperature","","Max","°C","70","70","70"]
["","Connection","","","mm","60","60","60"]
["","Mass flow (G20)","","Max","kg/h","20.9","31.3","20.9"]
["","Mass flow (G25)","","Max","kg/h","20.9","31.3","20.9"]
["","Mass flow (G31)","","Max","kg/h","20.5","30.6","20.5"]
["Casing","Colour","","","","RAL9010","RAL9010","RAL9010"]
["","Material","","","","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal"]
["Dimensions","Unit","Height","Casing","mm","590","590","590"]
["","","","Width","mm","450","450","450"]
["","","","Depth","mm","240","240","240"]
["Weight","Unit","","Empty","kg","30","30","30"]
["Space heating","General","","Seasonal space heating eff. class","","A","A","A"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]