{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":9,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-E6V / ERGA-EV7"]
[]
[]
[]
[]
["","","","","","EHVX04S23EA6V / ERGA04EAV37","EHVX04S23EJ6V / ERGA04EAV37","EHVX04S18EA6V / ERGA04EAV37","EHVX04S18EJ6V / ERGA04EAV37"]
["Heating capacity","Nom.","","","kW","4.36, 4.60","4.36, 4.60","4.36, 4.60","4.36, 4.60"]
["Cooling capacity","Nom.","","","kW","4.86, 4.52","4.86, 4.52","4.86, 4.52","4.86, 4.52"]
["Power input","Heating","","Nom.","kW","0.830, 1.26","0.830, 1.26","0.830, 1.26","0.830, 1.26"]
["","Cooling","","Nom.","kW","0.810, 1.36","0.810, 1.36","0.810, 1.36","0.810, 1.36"]
["","Domestic hot water from 10°C to 50°C","","Nom.","kWh","3.01","3.01","2.48","2.48"]
["Heat up time from 10°C to 50°C","hr","","","","1h40min","1h40min","1h28min","1h28min"]
["COP","","","","","5.23, 3.65","5.23, 3.65","5.23, 3.65","5.23, 3.65"]
["EER","","","","","5.98, 3.32","5.98, 3.32","5.98, 3.32","5.98, 3.32"]
["Domestic hot water heating","General","","Declared load profile","","XL","XL","L","L"]
["","Average climate","","Water heating energy efficiency class","","A","A","A","A"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.29","3.29","3.29","3.29"]
["","","","Seasonal space heating eff. class","","A++","A++","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.96","4.96","4.96","4.96"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++","A+++"]
["Notes","","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]