{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKCB-CV3"]
[]
[]
[]
[]
["","","","","EKCB07CAV3"]
["Dimensions","Unit","Width","mm","340"]
["","","Depth","mm","97.0"]
["","","Height","mm","360"]
["Casing","Material","","","Precoated sheet metal"]
["","Colour","","","White"]
["Weight","Unit","","kg","4.00"]
["Wiring connections","For power supply connection to optional *KHW* model + Q2L","Remark","","Cable section 2.5 mm2"]
["","","Määrä","","4 + GND"]
["","For connection with user interface","Remark","","100 mA, 0.75 mm² till 1.25 mm² (max length 500m)"]
["","","Quantity","","2"]
["Power supply","Phase","","","1~"]
["","Frequency","","Hz","50"]
["","Voltage","","V","230"]
["Current","Recommended fuses","","A","10"]
["Notes","","","","(1) - Equipment complying with EN/IEC 61000-3-12: European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current > 16A and ≤ 75A per phase"]
["","","","","(2) - Between *KCB*C* and *K2CB*C*"]
["","","","","(3) - Select diameter and type according to national and local regulations"]