{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHH2E-BV33"]
[]
[]
[]
[]
["","","","","","EKHH2E200BAV33"]
["Heat up time","Max.","","","hh:mm","07:05:00, See note 1, See note 2"]
["COP","","","","","3.28 (1)"]
["Domestic hot water","Output","","Nom","kW","1.89"]
["Equivalent hot water","Max","","","l","266"]
["Dimensions","Unit","","Height","mm","1744"]
["","","","Diameter","mm","650"]
["Weight","Unit","","Empty","kg","85"]
["","","","Full","kg","281"]
["","Packed unit","","","kg","105"]
["Installation place","","","","","Indoor"]
["IP class","","","","","IP-X4"]
["Compressor","Type","","","","Rotary non-inverter"]
["Refrigerant","Type","","","","R-134a"]
["","GWP","","","","1430.0"]
["","Charge","","","tCO2Eq","1.859"]
["","Charge","","","kg","1.3"]
["Heat pump","Casing","","Colour","","White body / grey top"]
["","","","Material","","Cover: EPP top finishing"]
["","Operation range","Ambient","Min.","°CDB","-7"]
["","","","Max.","°CDB","38"]
["","Defrost method","","","","Active with hot gas valve"]
["","Automatic defrost start","","","°C","-2"]
["","System pressure","","Max.","bar","7"]
["Tank","Operation range","Water side","Max.","°C","56"]
["","","","Min.","°C","10"]
["","Integrated heating element power","","Nom.","kW","1.5"]
["","Casing","","Colour","","White"]
["","","","Material","","Embossed ABS"]
["","Dimensions","Unit","Height","mm","1240"]
["","Installation","","Solar thermal connection possible","","No"]
["General","Product description","","Air-to-water heat pump","","Yes"]
["","Supplier/Manufacturer details","","Name and address","","E.L.I.C. - Via Pietro Zorutti 13/14/16, 33074 Fontanafredda ITALY"]
["Domestic hot water heating","General","","Declared load profile","","L"]
["","","","Water heating energy efficiency class","","A+"]
["","","","Thermostat temperature setting","°C","55"]
["Sound power level","Domestic hot water heating","","Outdoor unit","dBA","52"]
["","","","Indoor unit","dBA","53"]
["Domestic hot water heating","Average climate","","AEC (Annual electricity consumption)","kWh","752"]
["Energy Efficiency Range","","","","","A+ ~ F"]
["Heat pump","Power supply","","Phase","","1P"]
["","","","Frequency","Hz","50"]
["","","","Voltage","V","230"]
["","","","Maximum running current","A","2.4"]
["Tank","Power supply","","Phase","","1P"]
["","","","Frequency","Hz","50"]
["","","","Voltage","V","230"]
["Notes","","","","","(1) - Test at Ta DB/WB 7°C/6°C. According to EN 16147."]