{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":77,"n_cols":7,"rows_kept":77,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHHEU-CV37"]
[]
[]
[]
[]
["","","","","","EKHHEU200CV37","EKHHEU260CV37"]
["Heat up time","Max.","","","hh:mm","06:27:00","09:29:00"]
["COP","","","","","3.23","3.37"]
["Domestic hot water","Output","","Nom","kW","1.339","1249"]
["Equivalent hot water","Max","","","l","247","340"]
["Dimensions","Unit","","Height","mm","1607","1892"]
["","","","Diameter","mm","621","621"]
["Weight","Unit","","Empty","kg","85","97"]
["","","","Full","kg","277","347"]
["Dimensions","Unit","Height","Integrated on indoor unit","mm","1607","1892"]
["Weight","Packed unit","","","kg","96","109"]
["Installation place","","","","","Indoor","Indoor"]
["IP class","","","","","IP24","IP24"]
["Compressor","Type","","","","Rotary","Rotary"]
["Refrigerant","Type","","","","R-134a","R-134a"]
["Heat pump","Name","","","","EKHHEU200CV37","EKHHEU260CV37"]
["Refrigerant","GWP","","","","1430","1430"]
["","Charge","","","tCO2Eq","1.43","1.43"]
["","Charge","","","kg","1","1"]
["Heat pump","Heating capacity","","","kW","0.43","0.43"]
["","Casing","","Colour","","White","White"]
["","Dimensions","Unit","Height","mm","1607","1892"]
["","","","Width","mm","621","621"]
["","","","Depth","mm","621","621"]
["","Weight","","Unit","kg","85","97"]
["","","","Packed unit","kg","96","109"]
["","Installation place","","","","Indoor only","Indoor only"]
["","Installation","","IP class","","IP24","IP24"]
["","","","Distance from wall","mm","200","200"]
["","Operation range","Ambient","Min.","°CDB","-7","-7"]
["","","","Max.","°CDB","43","43"]
["","Sound pressure level","","Nom.","dBA","53","51"]
["","","","Night quiet mode","dBA","53.0","51"]
["","Refrigerant","","Type","","R-134A","R-134A"]
["","","","GWP","","1430","1430"]
["","","","Charge","tCO2Eq","1.43","1.43"]
["","","","Charge","kg","1","1"]
["","Defrost method","","","","Hot gas defrosting","Hot gas defrosting"]
["","System pressure","","Max.","bar","7","7"]
["Tank","Integrated heating element power","","Nom.","kW","1.5","1.5"]
["","Casing","","Colour","","White","White"]
["","","","Material","","Enamelled steel","Enamelled steel"]
["","Installation place","","","","Indoor only","Indoor only"]
["","Installation","","IP class","","IP24","IP24"]
["","","","Solar thermal connection possible","","No","No"]
["","","","Tank recirculation opening","","No","No"]
["General","Product description","","Air-to-water heat pump","","Yes","Yes"]
["","","","Model identifier","","EKHHEU200CV37","EKHHEU260CV37"]
["","Supplementary heater","","Type of energy input","","Electricity","Electricity"]
["","Supplier/Manufacturer details","","Name or trademark","","Daikin Europe N.V.","Daikin Europe N.V."]
["","LW(A) Sound power level (according to EN14825)","","Indoor","dBA","53","51"]
["Domestic hot water heating","General","","Declared load profile","","L","XL"]
["","","","Function to fix water heating during off peak hours","","Yes","Yes"]
["","","","Water heating energy efficiency class","","A+","A+"]
["","","","Thermostat temperature setting","°C","55","55"]
["Sound power level","Domestic hot water heating","","Outdoor unit","dBA","45","44"]
["","","","Indoor unit","dBA","53","51"]
["Domestic hot water heating","Average climate","","AEC (Annual electricity consumption)","kWh","761","1210"]
["","","","Qelec (Daily electricity consumption)","kWh","2.08","3.31"]
["","Cold climate","","AEC (Annual electricity consumption)","kWh","944","1496"]
["","","","Qelec (Daily electricity consumption)","kWh","2.59","4.10"]
["","Warm climate","","AEC (Annual electricity consumption)","kWh","631","1046"]
["","","","Qelec (Daily electricity consumption)","kWh","1.73","2.87"]
["Energy Efficiency Range","","","","","A+ ~ F","A+ ~ F"]
["Heat pump","Power supply","","Phase","","1P","1P"]
["","","","Frequency","Hz","50","50"]
["","","","Voltage","V","230","230"]
["","","","Maximum running current","A","8.5","8.5"]
["","","","Recommended field use","A","2.43","2.43"]
["Tank","Power supply","","Phase","","1P","1P"]
["","","","Frequency","Hz","50","50"]
["","","","Voltage","V","230","230"]