{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWC-B"]
[]
[]
[]
[]
["","","","","","EKHWC500BA"]
["Mounting","","","","","Floor"]
["Casing","Colour","","","","Traffic white (RAL9016) / Dark grey (RAL7011)"]
["","Material","","","","Impact resistant polypropylene"]
["Dimensions","Unit","Height","Tank","mm","1,660"]
["","","","Width","mm","790"]
["","","","Depth","mm","790"]
["Weight","Unit","","Empty","kg","69"]
["","","","Full","kg","569"]
["Tank","Water volume","","","l","477"]
["","Material","","","","Polypropylen"]
["","Maximum water temperature","","","°C","85"]
["","Energy efficiency class","","","","B"]
["Heat exchanger","Domestic hot water","","Quantity","","1"]
["","","","Tube material","","Stainless steel (DIN 1.4404)"]
["","","","Internal coil volume","l","23.8"]
["","","","Operating pressure","bar","6"]
["","","","Average specifc thermal output","W/K","2,450"]
["","Auxiliary solar heating","","Quantity","","1"]
["","","","Tube material","","Stainless steel (DIN 1.4404)"]
["","","","Internal coil volume","l","4"]
["","","","Operating pressure","bar","3"]
["","","","Average specifc thermal output","W/K","350"]
["Notes","","","","","(1) - Heatloss according to EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]
["","","","","","(5) - For tapping volume 140l -> 5820 Wh (bath) / 8kW heat pump"]
["","","","","","(6) - For tapping volume 90l -> 3660 Wh (bath) / 8kW heat pump"]
["","","","","","(7) - For tapping volume 140l -> 5820 Wh (bath) / 16kW heat pump"]
["","","","","","(8) - For tapping volume 90l -> 3660 Wh (bath) / 16kW heat pump"]