{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWP-PB"]
[]
[]
[]
[]
["","","","","","EKHWP300PB","EKHWP500PB"]
["Mounting","","","","","Floor","Floor"]
["Casing","Colour","","","","Traffic white (RAL9016) / Dark grey (RAL7011)","Traffic white (RAL9016) / Dark grey (RAL7011)"]
["","Material","","","","Impact resistant polypropylene","Impact resistant polypropylene"]
["Dimensions","Unit","Height","Tank","mm","1646","1658"]
["","","","Width","mm","595","790"]
["","","","Depth","mm","615","790"]
["Weight","Unit","","Empty","kg","56","82"]
["","","","Full","kg","350","559"]
["Tank","Water volume","","","l","294","477"]
["","Material","","","","Polypropylen","Polypropylen"]
["","Maximum water temperature","","","°C","85","85"]
["","Energy efficiency class","","","","B","B"]
["Heat exchanger","Domestic hot water","","Quantity","","1","1"]
["","","","Tube material","","Stainless steel (DIN 1.4404)","Stainless steel (DIN 1.4404)"]
["","","","Internal coil volume","l","27.8","29.0"]
["","","","Operating pressure","bar","10.0","10.0"]
["","Charging","","Quantity","","1","1"]
["","","","Tube material","","Stainless steel (DIN 1.4404)","Stainless steel (DIN 1.4404)"]
["","","","Internal coil volume","l","12.9","18.1"]
["","","","Operating pressure","bar","6.0","6.0"]
["","Auxiliary solar heating","","Quantity","","","1"]
["","","","Tube material","","","Stainless steel (DIN 1.4404)"]
["","","","Internal coil volume","l","","3.9"]
["","","","Operating pressure","bar","","3.0"]
["Notes","","","","","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]
["","","","","","(5) - For tapping volume 140l -> 5820 Wh (bath) / 8kW heat pump","(5) - For tapping volume 140l -> 5820 Wh (bath) / 16kW heat pump"]
["","","","","","(6) - For tapping volume 90l -> 3660 Wh (bath) / 8kW heat pump","(6) - For tapping volume 90l -> 3660 Wh (bath) / 16kW heat pump"]
["Energy Efficiency Range","","","","","A+ ~ F"]
["Notes","","","","","(7) - For tapping volume 140l -> 5820 Wh (bath) / 16kW heat pump"]
["","","","","","(8) - For tapping volume 90l -> 3660 Wh (bath) / 16kW heat pump"]
["","","","","","(9) - Heat exchanger connected in parallel, TKW= 10°C/ TWW= 45°C/ TSP= 65°C/ Pload= 35kW/ Tflow= 80°C"]
["","","","","","(10) - TKW= 10°C/ TWW= 45°C/ TSP= 65°C/ Pload= 35kW/ Tflow= 80°C"]