{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKMBUHC3V3"]
[]
[]
[]
[]
["","","","","EKMBUHCA3V3"]
["Dimensions","Unit","Width","mm","250"]
["","","Depth","mm","210"]
["","","Height","mm","560"]
["Casing","Material","","","Precoated sheet metal"]
["","Colour","","","White"]
["Weight","Unit","","kg","11.0"]
["Electric heater","Power supply","Frequency","Hz","50"]
["","","Voltage","V","230"]
["","","Name","","3V3"]
["","","Phase","","1~"]
["Notes","","","","(1) - Equipment complying with EN/IEC 61000-3-12: European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current > 16A and ≤ 75A per phase"]
["","","","","(2) - Refer to installation manual or drawing 4D097266"]
["","","","","(3) - Select diameter and type according to national and local regulations"]