{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":78,"n_cols":8,"rows_kept":78,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKOMB-AH"]
[]
[]
[]
[]
["","","","","","EKOMB22AAV1H","EKOMB28AAV1H","EKOMB33AAV1H"]
["Gas","Connection","","Diameter","mm","","15"]
["","Consumption (G20)","","Min","m³/h","","0.74"]
["","","","Max","m³/h","","2.91"]
["","Consumption (G25)","","Min","m³/h","","0.85"]
["","","","Max","m³/h","","3.36"]
["","Consumption (G31)","","Min","m³/h","","0.28"]
["","","","Max","m³/h","","1.11"]
["","NOx class","","","","","6"]
["","NOx level (G20)","","","mg/kWh","","44"]
["Central heating","Heat input Qn (net calorific value)","Nom","Min","kW","","7.1"]
["","","","Max","kW","","23.7"]
["","Heat input Qn (gross calorific value)","Nom","Min","kW","","7.9"]
["","","","Max","kW","","26.3"]
["","Output Pn at 80/60°C","","Nom","kW","","22.8"]
["","Output at 37/30°C","","Nom","kW","","7.7"]
["","Water temperature","","Max","°C","","90"]
["Domestic hot water","Heat input (net calorific value) Qnw","Nom","Min","kW","","7.1"]
["","","","Max","kW","","28.0"]
["","Heat input (gross calorific value) Qnw","Nom","Min","kW","","7.9"]
["","","","Max","kW","","31.1"]
["","Comfort class (EN13203)","","","","","XL"]
["","Temperature","","Max","°C","","65"]
["Space heating","General","","ηs (Seasonal space heating efficiency)","%","","92"]
["","","","Seasonal space heating eff. class","","","A"]
["Supply air","Concentric","","","","","60/100"]
["Flue gas","Temperature","","Max","°C","","90"]
["","Mass flow (G20)","","Max","kg/h","","46.8"]
["","Mass flow (G25)","","Max","kg/h","","46.8"]
["","Mass flow (G31)","","Max","kg/h","","46.1"]
["Casing","Colour","","","","","RAL9010"]
["","Material","","","","","Precoated sheet metal"]
["Dimensions","Unit","Height","Casing","mm","","650"]
["Domestic hot water heating","General","","Declared load profile","","","XL"]
["","","","Water heating energy efficiency class","","","A"]
["Gas","Connection","","Diameter","mm","15","","15"]
["","Consumption (G20)","","Min","m³/h","0.58","","0.75"]
["","","","Max","m³/h","2.29","","3.39"]
["","Consumption (G25)","","Min","m³/h","0.67","","0.86"]
["","","","Max","m³/h","2.65","","3.93"]
["","Consumption (G31)","","Min","m³/h","0.22","","0.28"]
["","","","Max","m³/h","0.87","","1.29"]
["","NOx class","","","","6","","6"]
["","NOx level (G20)","","","mg/kWh","33","","34"]
["Central heating","Heat input Qn (net calorific value)","Nom","Min","kW","5.6","","7.2"]
["","","","Max","kW","18.7","","27.3"]
["","Heat input Qn (gross calorific value)","Nom","Min","kW","6.2","","8.0"]
["","","","Max","kW","20.8","","30.3"]
["","Output Pn at 80/60°C","","Nom","kW","17.8","","26.3"]
["","Output at 37/30°C","","Nom","kW","6.0","","7.8"]
["","Water temperature","","Max","°C","90","","90"]
["Domestic hot water","Heat input (net calorific value) Qnw","Nom","Min","kW","5.6","","7.2"]
["","","","Max","kW","22.1","","32.7"]
["","Heat input (gross calorific value) Qnw","Nom","Min","kW","6.2","","8.0"]
["","","","Max","kW","24.6","","36.3"]
["","Comfort class (EN13203)","","","","L","","XL"]
["","Temperature","","Max","°C","65","","65"]
["Supply air","Concentric","","","","60/100","","60/100"]
["Flue gas","Temperature","","Max","°C","90","","90"]
["","Connection","","","mm","60","","60"]
["","Mass flow (G20)","","Max","kg/h","37.1","","53.6"]
["","Mass flow (G25)","","Max","kg/h","37.1","","53.6"]
["","Mass flow (G31)","","Max","kg/h","36.4","","54.4"]
["Casing","Colour","","","","RAL9010","","RAL9010"]
["","Material","","","","Precoated sheet metal","","Precoated sheet metal"]
["Dimensions","Unit","Height","Casing","mm","590","","710"]
["","","","Width","mm","450","","450"]
["","","","Depth","mm","240","","240"]
["Weight","Unit","","Empty","kg","30","","36"]
["Domestic hot water heating","General","","Declared load profile","","L","","XL"]
["","","","Water heating energy efficiency class","","A","","A"]
["Space heating","General","","Seasonal space heating eff. class","","A","","A"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]