{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":11,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKOMBG-A"]
[]
[]
[]
[]
["","","","","","EKOMBG22ABV1","EKOMBG22AAV1","EKOMBG28AAV1","EKOMBG28ABV1","EKOMBG33ABV1","EKOMBG33AAV1"]
["Gas","Connection","","Diameter","mm","15","15","15","15","15","15"]
["","Consumption (G20)","","Min","m³/h","0.58","0.58","0.74","0.74","0.79","0.79"]
["","","","Max","m³/h","2.42","2.42","3.02","3.02","3.39","3.39"]
["","Consumption (G25)","","Min","m³/h","0.62","0.62","0.84","0.84","0.89","0.89"]
["","","","Max","m³/h","2.82","2.82","3.46","3.46","3.92","3.92"]
["","Consumption (G31)","","Min","m³/h","0.21","0.21","0.29","0.29","0.30","0.30"]
["","","","Max","m³/h","0.94","0.94","1.19","1.19","1.29","1.29"]
["","NOx class","","","","6","6","6","6","6","6"]
["","NOx level (G20)","","","mg/kWh","28","28","27","27","36","36"]
["Central heating","Heat input Qn (net calorific value)","Nom","Min","kW","5.5","5.5","7.1","7.1","7.6","7.6"]
["","","","Max","kW","23.3","23.3","29.1","29.1","32.7","32.7"]
["","Heat input Qn (gross calorific value)","Nom","Min","kW","6.1","6.1","7.9","7.9","8.4","8.4"]
["","","","Max","kW","25.9","25.9","32.3","32.3","36.3","36.3"]
["","Output Pn at 80/60°C","","Min","kW","6.0","6.0","7.6","7.6","8.3","8.3"]
["","","","Nom","kW","22.6","22.6","28.2","28.2","32.0","32.0"]
["","Output at 37/30°C","","Nom","kW","6.0","6.0","7.6","7.6","8.3","8.3"]
["","Water temperature","","Max","°C","90","90","90","90","90","90"]
["Domestic hot water","Heat input (net calorific value) Qnw","Nom","Min","kW","5.5","5.5","7.1","7.1","7.6","7.6"]
["","","","Max","kW","23.3","23.3","29.1","29.1","32.7","32.7"]
["","Heat input (gross calorific value) Qnw","Nom","Min","kW","6.1","6.1","7.9","7.9","8.4","8.4"]
["","","","Max","kW","25.9","25.9","23.3","23.3","36.3","36.3"]
["","Comfort class (EN13203)","","","","L","L","XL","XL","XL","XL"]
["","Temperature","","Max","°C","65","65","65","65","65","65"]
["Supply air","Concentric","","","","60/100","60/100","60/100","60/100","60/100","60/100"]
["Flue gas","Temperature","","Max","°C","70","70","70","70","70","70"]
["","Connection","","","mm","60","60","60","60","60","60"]
["","Mass flow (G20)","","Max","kg/h","38.9","38.9","48.6","48.6","54.4","54.4"]
["","Mass flow (G25)","","Max","kg/h","38.9","38.9","48.6","48.6","54.4","54.4"]
["","Mass flow (G31)","","Max","kg/h","38.2","38.2","47.9","47.9","53.6","53.6"]
["Casing","Colour","","","","RAL9010","RAL9010","RAL9010","RAL9010","RAL9010","RAL9010"]
["","Material","","","","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal"]
["Dimensions","Unit","Height","Casing","mm","590","590","650","650","710","710"]
["","","","Width","mm","450","450","450","450","450","450"]
["","","","Depth","mm","240","240","240","240","240","240"]
["Weight","Unit","","Empty","kg","30","30","33","33","36","36"]
["Domestic hot water heating","General","","Declared load profile","","L","L","XL","XL","XL","XL"]
["","","","Water heating energy efficiency class","","A","A","A","A","A","A"]
["Space heating","General","","Seasonal space heating eff. class","","A","A","A","A","A","A"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]