{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKSH-P"]
[]
[]
[]
[]
["","","","","EKSH26P1","EKSH26P"]
["Absorber","","","","Harp-shaped copper pipe register with laser-welded highly selective coated aluminium plate","Harp-shaped copper pipe register with laser-welded highly selective coated aluminium plate"]
["Stand still temperature","Max.","","°C","192","192"]
["Dimensions","Unit","Width","mm","2,000","85"]
["","","Depth","mm","85","1,300"]
["","","Height","mm","1,300","2,000"]
["Weight","Unit","","kg","42","42"]
["Operating pressure","Max.","","bar","6","6"]
["Surface","Aperture","","m²","2.360","2.360"]
["","Absorber","","m²","2.36","2.35"]
["","Outer","","m²","2.60","2.60"]
["Mounting","","","","Horizontal","Horizontal"]
["Glazing","","","","Single pane safety glass, transmission +/- 92%","Single pane safety glass, transmission +/- 92%"]
["Allowed roof angle","Max.","","°","80","80"]
["","Min.","","°","15","15"]
["Coating","","","","Micro-therm (absorption max. 96%, Emission ca. 5% +/-2%)","Micro-therm (absorption max. 96%, Emission ca. 5% +/-2%)"]
["Volume","l","","","2.1","2.1"]
["Thermal performance","Zero loss collector efficiency η0","","%","0.710","0.784"]
["","Heat loss coefficient a1","","W/m².K","4.300","4.250"]
["","Temperature dependence of the heat loss coefficient a2","","W/m².K²","0.006","0.007"]
["","Thermal capacity","","kJ/K","6.5","6.5"]