{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELSHB-E / ERRA08-12EW1"]
[]
[]
[]
[]
["","","","","","ELSHB12P30EF / ERRA08EAW1","ELSHB12P50EF / ERRA08EAW1","ELSHB12P30EF / ERRA10EAW1","ELSHB12P50EF / ERRA10EAW1","ELSHB12P30EF / ERRA12EAW1","ELSHB12P50EF / ERRA12EAW1"]
["Heating capacity","Min.","","","kW","3.45","3.45","3.45","3.45","3.45","3.45"]
["","Nom.","","","kW","6.17","6.17","6.17","6.17","6.17","6.17"]
["","Max.","","","kW","7.95","7.95","9.25","9.25","9.97","9.97"]
["Power input","Heating","","Min.","kW","0.70","0.70","0.70","0.70","0.70","0.70"]
["","","","Nom.","kW","1.21","1.21","1.21","1.21","1.21","1.21"]
["","","","Max.","kW","1.63","1.63","1.98","1.98","2.21","2.21"]
["","Domestic hot water from 10°C to 50°C","","Nom.","kWh","3.44","4.65","3.44","4.65","3.44","4.65"]
["Heat up time from 10°C to 50°C","hr","","","","2h29min","3h45min","2h29min","3h45min","2h29min","3h45min"]
["COP","","","","","5.10","5.10","5.10","5.10","5.10","5.10"]
["Domestic hot water heating","General","","Declared load profile","","L","XL","L","XL","L","XL"]
["","Average climate","","Water heating energy efficiency class","","A+","A+","A+","A+","A+","A+"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.42","3.42","3.43","3.43","3.53","3.53"]
["","","","Seasonal space heating eff. class","","A++","A++","A++","A++","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.81","4.81","4.84","4.84","4.84","4.84"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++","A+++","A+++","A+++"]
["Notes","","","","","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C"]
["","","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(3) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(3) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(3) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(3) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(3) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511"]
["","","","","","(4) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(4) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(4) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(4) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(4) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(4) - Test at Ta DB/WB 7°C/6°C. According to EN 16147."]
["","","","","","(5) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(5) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(5) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(5) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(5) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(5) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed"]