{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELSX-E"]
[]
[]
[]
[]
["","","","","","ELSX12P50EF","ELSX12P30EF","ELSX12P50EG","ELSX12P30EG"]
["Casing","Colour","","","","Traffic white (RAL9016) / Traffic black (RAL9017)","Traffic white (RAL9016) / Traffic black (RAL9017)","Traffic white (RAL9016) / Traffic black (RAL9017)","Traffic white (RAL9016) / Traffic black (RAL9017)"]
["","Material","","","","Impact resistant polypropylene","Impact resistant polypropylene","Impact resistant polypropylene","Impact resistant polypropylene"]
["Dimensions","Unit","","Height","mm","1,910","1,893","1,910","1,891"]
["","","","Width","mm","792","594","792","594"]
["","","","Depth","mm","817","680","817","680"]
["Weight","Unit","","","kg","91.0","76.0","112","91.0"]
["PED","Category","","","","Category II","Category II","Category II","Category II"]
["Refrigerant","Type","","","","R-32","R-32","R-32","R-32"]
["Sound power level","Nom.","","","dBA","44.7","44.7","44.7","44.7"]
["Sound pressure level","Nom.","","","dBA","36.8","36.8","36.8","36.8"]
["Operation range","Heating","Water side","Min.","°C","15 (3)","15 (3)","15 (3)","15 (3)"]
["","","","Max.","°C","65 (3)","65 (3)","65 (3)","65 (3)"]
["","Cooling","Ambient","Min.","°CDB","10 (3)","10 (3)","10 (3)","10 (3)"]
["","","Water side","Min.","°C","5 (3)","5 (3)","5 (3)","5 (3)"]
["","","","Max.","°C","22 (3)","22 (3)","22 (3)","22 (3)"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","230","230","230","230"]
["Notes","","","","","(1) - Operation area is extended to lower flow rates depending on operation mode - refer to ESP curve.","(1) - Operation area is extended to lower flow rates depending on operation mode - refer to ESP curve.","(1) - Operation area is extended to lower flow rates depending on operation mode - refer to ESP curve.","(1) - Operation area is extended to lower flow rates depending on operation mode - refer to ESP curve."]
["","","","","","(2) - Heatloss according to EN12897","(2) - Heatloss according to EN12897","(2) - Heatloss according to EN12897","(2) - Heatloss according to EN12897"]
["","","","","","(3) - For more details, see operation range drawing","(3) - For more details, see operation range drawing","(3) - For more details, see operation range drawing","(3) - For more details, see operation range drawing"]