{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPBXU14A9W / EPSK12-14AW1"]
[]
[]
[]
[]
["","","","","","EPBXU14AF9W / EPSK12ARW1","EPBXU14AF9W / EPSK14ARW1"]
["Heating capacity","Nom.","","","kW","10.2 (1)","10.2 (1)"]
["","Max.","","","kW","11.99 (2)","13.34 (2)"]
["Cooling capacity","Nom.","","","kW","9.37 (3), 6.74 (4)","11.3 (3), 6.74 (4)"]
["Power input","Heating","","Nom.","kW","1.86 (1)","1.86 (1)"]
["","","","Max.","kW","3.51 (5)","3.98 (5)"]
["","Cooling","","Nom.","kW","2.64 (3), 1.12 (4)","3.45 (3), 1.12 (4)"]
["COP","","","","","5.50 (1)","5.50 (1)"]
["EER","","","","","3.55 (3), 6.04 (4)","3.28 (3), 6.04 (4)"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","4.04","3.84"]
["","","","Seasonal space heating eff. class","","A+++","A+++"]
["","Average climate water outlet 35°C","General","SCOP","","5.14","4.96"]
["","","","Seasonal space heating eff. class","","A+++","A+++"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Notes","","","","","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(2) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C"]
["","","","","","(3) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(3) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB"]
["","","","","","(4) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(4) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB"]
["","","","","","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511"]