{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSK06-10AV3"]
[]
[]
[]
[]
["","","","","","EPSK06ARV3","EPSK08ARV3","EPSK10ARV3"]
["Dimensions","Unit","","Height","mm","1,123","1,123","1123"]
["","","","Width","mm","1,330","1,330","1330"]
["","","","Depth","mm","604","604","604"]
["Weight","Unit","","","kg","174","174","174"]
["Fan","Air flow rate","Heating","High","m³/min","75.7","75.7","75.7"]
["","","Cooling","High","m³/min","75.7","75.7","75.7"]
["Operation range","Cooling","","Min.","°CDB","10","10","10"]
["","","","Max.","°CDB","43","43","43"]
["","Domestic hot water","","Min.","°CDB","-28","-28","-28"]
["","","","Max.","°CDB","40","40","40"]
["Sound power level","Heating","","Nom.","dBA","45 (1)","45 (1)","47 (1)"]
["","Cooling","","Nom.","dBA","52.2 (2)","53 (2)","53.2 (2)"]
["Sound pressure level","Heating","","Nom.","dBA","32.6 (1)","32.4 (1)","32.8 (1)"]
["","Cooling","","Nom.","dBA","36.9 (2)","37.2 (2)","37.3 (2)"]
["Refrigerant","Type","","","","R-290","R-290","R-290"]
["","GWP","","","","3","3","3"]
["","Charge","","","tCO2Eq","0.003","0.003","0.003"]
["","Charge","","","kg","1","1","1"]
["Piping connections","Level difference","IU - OU","Max.","m","10","10","10"]
["Power supply","Name","","","","V3","V3","V3"]
["","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","230","230","230"]
["Current","Recommended fuses","","","A","25","25","25"]
["Notes","","","","","(1) - Measured at LWC 47-55°C ; Ta DB/WB 7°C/6°C.","(1) - Measured at LWC 47-55°C ; Ta DB/WB 7°C/6°C.","(1) - Measured at LWC 47-55°C ; Ta DB/WB 7°C/6°C."]
["","","","","","(2) - Measured at LWC 12-7°C ; Ta 35°C.","(2) - Measured at LWC 12-7°C ; Ta 35°C.","(2) - Measured at LWC 12-7°C ; Ta 35°C."]
["","","","","","(3) - 1 1/4\" field piping","(3) - 1 1/4\" field piping","(3) - 1 1/4\" field piping"]
["","","","","","(4) - 1 1/2\" field piping","(4) - 1 1/2\" field piping","(4) - 1 1/2\" field piping"]